Data/hora: 16/06/2024 09:12:36

Provedor de dados: | 5
País: | France

Título:

Étude du comportement non-linéaire d'une colle dans un assemblage

Analysis of the non-linear behaviour of an adhesive in an assembly

Autores: | Cognard, Jean-yves; Sohier, Laurent; Davies, Peter; Gineste, Bernard.
Data: | 2006-05
Ano: | 2006
Palavras-chave: | Ssemblages collés; Modélisation; Essais; Comportement non-linéaire; Composites; Adhesive bonding; Model; Tests; Non linear behaviour; Composite.
Resumo: | The objective of this study is to define a reliable tool for dimensioning of adhesively bonded assemblies, particularly for marine and underwater applications. A modified “Arcan” fixture, suited for the study of the behavior of bonded metal-metal assemblies, was developed in order to focus on the analysis of the behavior of the adhesive in thin films. To analyze the kinematics of the deformation of the adhesive joint non-contact extensometry techniques were employed. Thus various characteristics of the non-linear behavior of the adhesive were observed. The first results obtained for mixed assemblies (steel, aluminium, composite substrates) show similar behaviour of the adhesive using the proposed procedure. Furthermore, quality controls by DSC, and studies of curing by DMA have been performed to verify the bonding procedure.
Tipo: | Text
Idioma: | Francês

Identificador:

https://archimer.ifremer.fr/doc/00480/59156/61785.pdf

DOI:10.1051/meca:2006040

https://archimer.ifremer.fr/doc/00480/59156/

Editor: | EDP Sciences
Formato: | application/pdf
Fonte: | Mécanique &amp; Industries (1296-2139) (EDP Sciences), 2006-05 , Vol. 7 , N. 3 , P. 265-276

Fonte:

info:eu-repo/semantics/openAccess

restricted use