Data/hora: 16/06/2024 09:12:56

Provedor de dados: 	5	
País: 	France	
Título: 	Remaniements sédimentaires superficiels sur l'estran occidental de la baie du Mont Saint-Michel	
Autores: 	Bonnot-courtois, C; Bassoullet, Philippe; Tessier, B; Cayocca, Florence; Le Hir, Pierre; Baltzer, A.	
Data: 	2008-02	
Ano: 	2008	
Palavras-chave: 	Sediment transport; Numerical model; Erosion sedimentation budget; "In situ" measurements; Tidal sandy mud flat; Transport sédimentaire; Modèle numérique; Bilan érosion sédimentation; Mesures in situ; Estran sablo vaseux.	
Resumo: 	In order to define and quantify the rhythm and amplitude of the processes of erosion and sedimentation on broad tidal flats, in situ measurements of sediment elevation have been performed in the western part of the Mont-Saint-Michel bay. The amplitude of reworking is generally low (&lt; ± 5 cm), and variable from west to east. The wind influence on tidal currents and surficial reworking emphasizes erosion phases rapidly followed by accretion of similar amplitude on the whole tidal flat. A numerical model for hydrodynamics and sediment transport is applied to Mont Saint Michel Bay, where ecological concerns are related to sediment transfers.	
Tipo: 	Text	
Idioma: 	Francês	
Identificador: 	http://archimer.ifremer.fr/doc/2008/publication-6279.pdf

DOI:10.3166/ejece.12.51-65	
Editor: 	Lavoisier	
Relação: 	http://archimer.ifremer.fr/doc/00000/6279/	
Formato: 	application/pdf	
Fonte: 	Revue Européenne de Génie Civil (Lavoisier), 2008-02 , Vol. 12 , N. 1-2 , P. 51-65	
Fonte: 	2008 Lavoisier