Data/hora: 07/06/2024 02:15:31

Provedor de dados: 	5	
País: 	France	
Título: 	A comprehensive assessment of turbulence at a tidal-stream energy site influenced by wind-generated ocean waves	
Autores: 	Thiébaut, Maxime; Filipot, Jean-francois; Maisondieu, Christophe; Damblans, Guillaume; Duarte, Rui; Droniou, Eloi; Chaplain, Nicolas; Guillou, Sylvain.	
Data: 	2020-01	
Ano: 	2020	
Palavras-chave: 	Turbulence; Tidal energy; Wave; Doppler noise; ADCP; Alderney Race.	
Resumo: 	Velocity measurements collected by an upward-looking acoustic Doppler current profiler were used to provide the first study of ambient turbulence in Alderney Race. Turbulence metrics were estimated at mid-depth during peak flooding and ebbing tidal conditions. The dissipation rate ε and the integral lengthscale (L) were estimated using two independent methods: the spectral method and the structure function method. The spectral method provided ε and (L) estimates with standard deviations twice lower than that obtained from the structure function method. Removal of wave and Doppler noise-induced bias when estimating the dissipation rate was shown to be a crucial step in turbulence characterization. It allowed for a significant refining in (L) estimates derived from the spectral and structure function methods of 35 and 20 respectively. The integral lengthscale was found to be 2–3 times the local water depth. It is considered that these findings could be valuable for current turbine designers, helping them optimizing their designs as well as improving loading prediction through the lifetime of the machines.	
Tipo: 	Text	
Idioma: 	Inglês	
Identificador: 	https://archimer.ifremer.fr/doc/00592/70394/68478.pdf

DOI:10.1016/j.energy.2019.116550

https://archimer.ifremer.fr/doc/00592/70394/	
Editor: 	Elsevier BV	
Formato: 	application/pdf	
Fonte: 	Energy (0360-5442) (Elsevier BV), 2020-01 , Vol. 191 , P. 116550 (12p.)	
Fonte: 	info:eu-repo/semantics/openAccess

restricted use