Data/hora: 06/06/2024 01:31:42

Provedor de dados: | 5
País: | France
Título: | Biofouling protection for marine underwater observatories sensors
Autores: | Delauney, Laurent; Compere, Chantal; Lehaitre, Michel.
Data: | 2009
Ano: | 2009
Resumo: | These days, many marine autonomous environment monitoring networks are set up in the world. Such systems take advantage of existing superstructures such as offshore platforms, lightships, piers, breakwaters or are placed on specially designed buoys or deep sea fix stations. The major goal for these equipments is to provide in real time reliable measurements without costly frequent maintenance. These autonomous monitoring systems are affected by a well known phenomena in seawater condition which is biofouling. Consequently, such system without efficient biofouling protection is hopeless. This protection must be applied to the sensors and to the underwater acoustic communication equipments.
Tipo: | Text
Idioma: | Inglês

Identificador:

http://archimer.ifremer.fr/doc/00107/21801/20176.pdf

DOI:http://dx.doi.org/10.1109/OCEANSE.2009.5278199

Editor: | Ieee
Relação: | http://archimer.ifremer.fr/doc/00107/21801/
Formato: | application/pdf
Fonte: | Oceans 2009 - Europe, Vols 1 And 2 (0197-7385) (Ieee), 2009 , P. 1069-1072
Fonte: | Copyright 2013 IEEE - All rights reserved.