Data/hora: 13/06/2024 03:40:02

Provedor de dados: | 5
País: | France
Título: | Study of high frequency measurements from the MesuRho mooring
Autores: | Fuchs, Rosalie; Pairaud, Ivane.
Data: | 2014-01
Ano: | 2014
Palavras-chave: | MesuRho; Code qualité; Correction des données; Analyse et traitement de données; Filtrage; ACP; Fourier; Évènement de vent d'Est; MesuRho; Quality code; Data corrections; Data and treatments analysis; Filtering; PCA; Fourier; Storm event.
Resumo: | The high frequency MesuRho station, part of the MAREL network and located at the mouth of the Rhone River is presented. Measures sometimes show bias signs, drift or double, so that a graphical interface was implemented to quickly visualize data and eventually correct them. Original data set and corrected data for 2009-2013 are presented, the methods of corrections provided are detailed. Finally an example of a storm event study (under strong south east wind) between the 4th and the 7th of March 2013 is presented and some prospects to improve data management are proposed.
Tipo: | Text
Idioma: | Inglês

Identificador:

http://archimer.ifremer.fr/doc/00226/33697/32082.pdf

http://archimer.ifremer.fr/doc/00226/33697/

Relação: | info:eu-repo/grantAgreement/EC/FP7/287600/EU//PERSEUS
Formato: | application/pdf

Fonte:

2014 Ifremer

info:eu-repo/semantics/openAccess

restricted use