Data/hora: 05/06/2024 10:00:20

Provedor de dados: 	5	
País: 	France	
Título: 	Development and validation of the new ProvBioII float	
Autores: 	Leymarie, Edouard; Poteau, Antoine; Andre, Xavier; Besson, F; Brault, Patrice; Claustre, Herve; David, Arnaud; D'Ortenzio, Fabrizio; Dufour, A; Lavigne, Heloise; Le Reste, Serge; Le Traon, Pierre-yves; Migon, Christophe; Nogre, David; Obolensky, G; Penkerc'H, C; Sagot, Jerome; Schaeffer, Christophe; Schmechtig, C; Taillandier, V.	
Data: 	2013-06	
Ano: 	2013	
Resumo: 	In the last ten years, a productive collaboration has grown between the Laboratoire d’Océanographie de Villefranche (LOV), NKE and IFREMER to implement biogeochemical sensors on profiling floats. A first project (2003) was dedicated to the design of the so-called ProvBio floats (models A and B) that consisted of a PROVOR-CTS3 float instrumented with three new optical sensors: a Wetlabs transmissometer (C-Rover), a 3-wavelength Satlantic radiometer (OCR-503) and an “ECO3” Wetlabs sensor, measuring chlorophyll-a fluorescence, colored dissolved organic matter and particle backscattering coefficients (see First Success of ProvBio floats, Coriolis Letter n°5). Then, the integration of biogeochemical sensors continued in the framework of ProNuts project (2009, autonomously profiling the nitrate concentrations in the ocean: the pronuts project, Coriolis Letter n°8), by equipping a PROVOR with a nitrate concentration sensor. In parallel within the framework of the Carbocean EU project, the ProvCarbon and ProvDo floats were developed as in 2006 by fitting on a PROVOR a C-Rover and a 3830 Aanderaa optode, respectively. They were used to investigate new tools to assess marine carbon sources and sinks. These initial developments have led to a first invaluable dataset and to subsequent papers (Xing et al. 2012, Xing et al. 2011) and report (IOCCG 2011). Nevertheless, the above projects have grown partially dissociated, as related to specific and project-related needs, while a more integrated solution may have a lot of advantages. Undoubtedly, the scientific exploitation of data would be strongly improved if a unique multidisciplinary float, able to measure all accessible parameters, was available. Such a multidisciplinary float would also strongly reduce costs, by sharing the float itself, and by reducing deployment, validation and communication costs. The idea to merge all these sensors on the same profiling float was thus at the origin of the ProvBioII float project, which was developed in the framework of the remOcean and NAOS programs.	
Tipo: 	Text	
Idioma: 	Inglês	
Identificador: 	http://archimer.ifremer.fr/doc/00219/32989/31438.pdf

http://archimer.ifremer.fr/doc/00219/32989/	
Editor: 	Mercator Ocean	
Relação: 	info:eu-repo/grantAgreement/EC/FP7/211597/EU//EURO ARGO	
Formato: 	application/pdf	
Fonte: 	Mercator Ocean - quaterly newsletter (Mercator Ocean), 2013-06 , Vol. 48 , P. 26-30	
Fonte: 	info:eu-repo/semantics/openAccess

restricted use