Data/hora: 14/06/2024 06:02:52

Provedor de dados: | 5
País: | France
Título: | A new open cableb infrastructure in MEDSEA
Autores: | Leon, Pierre; Drogou, Jean-francois; Chenot, Damien; Leveque, C.; Martinossi, Henri; Massol, Alain; Rigaud, Vincent; Santarelli, Dominique; Valdy, Pierre; Gojak, Carl; Bernardet, Karim; Hafidi, Zouhir; Lenault, Yannick; Mahiouz, Karim; Deschamps, Anne; Hello, Y.; Lefevre, D.; Tamburini, C.; Destelle, J. J.
Data: | 2011
Ano: | 2011
Resumo: | Recently the ANTARES Neutrino telescope's Infrastructure in the deep Mediterranean Sea, has been extended by a Secondary Junction Box. The main emphasis has been to provide basic power and communications capability for new scientific cabled observatories. This new infrastructure provides unprecedented amounts of power and two-way bandwidth to access and control instrument networks in the oceans. This new development allows cabled observatory to connect the seafloor to the Internet via real-time, two-way highspeed communications. This design gives researchers new capabilities beyond the reach of traditional oceanography. Ocean scientists can run deep-water experiments from labs and universities anywhere around the world. Three different underwater observatories are already been connected at this Secondary Junction Box. This paper presents this new Infrastructure which has been deployed by the R/V Pourquoi Pas? and connected by the IFREMER's ROV VICTOR6000. After a technical description of the system, we detailled an overview of the complete deployment at sea.
Tipo: | Text
Idioma: | Inglês
Identificador: | http://archimer.ifremer.fr/doc/00050/16173/13658.pdf
Editor: | Ieee
Relação: | http://archimer.ifremer.fr/doc/00050/16173/
Formato: | application/pdf
Fonte: | 2011 Ieee - Oceans Spain (0197-7385) (Ieee), 2011 , P. -
Fonte: | 2011 IEEE