Data/hora: 01/06/2024 07:54:05

Provedor de dados: 	5	
País: 	France	
Título: 	Experimental study of coherent flow structures past a wall-mounted square cylinder	
Autores: 	Ikhennicheu, Maria; Germain, Gregory; Druault, Philippe; Gaurier, Benoit.	
Data: 	2019-06	
Ano: 	2019	
Palavras-chave: 	Turbulence; Experimental trials; Wall-mounted cylinder; PIV; LDV; POD; Lamb-Oseen.	
Resumo: 	In high flow velocity areas like those suitable for tidal applications, turbulence intensity is high and flow variations may have a major impact on tidal turbines behaviour. Large boils that can be observed at the sea surface are emitted from the sea floor and may interact with the tidal turbines. These boils have then to be characterized. The Reynolds number, based on the rugosity height and the mean flow velocity, is rather high in this context: Re ¼ 2:5 107. For that purpose, experiments are carried out in a flume tank with Re as high as achievable in Froude similitude (in the tank: Re ¼ 2:5  105 and Fr ¼ 0:23) in order to study coherent flow structures emitted behind seabed obstacles. The obstacle is here a canonical square wall-mounted cylinder chosen to be representative of specific in-situ bathymetric variations. Using PIV and LDV measurements, the flow past the cylinder is investigated. Using a POD filter, large coherent structures are identified and their trajectories are analysed. By means of a Lamb-Oseen profile approximation, properties of these structures are determined. The formation mechanism of such structures is discussed in this paper and their behaviour is characterized. It is assumed that vortices periodically shed from the obstacle interact and generate hairpin structures.	
Tipo: 	Text	
Idioma: 	Inglês	
Identificador: 	https://archimer.ifremer.fr/doc/00494/60527/64189.pdf

DOI:10.1016/j.oceaneng.2019.04.043

https://archimer.ifremer.fr/doc/00494/60527/	
Editor: 	Elsevier BV	
Formato: 	application/pdf	
Fonte: 	Ocean Engineering (0029-8018) (Elsevier BV), 2019-06 , Vol. 182 , P. 137-146	
Fonte: 	info:eu-repo/semantics/openAccess

restricted use