Data/hora: 01/06/2024 02:46:28

Provedor de dados: 	5	
País: 	France	
Título: 	A new device to follow temporal variations of oxygen demand in deltaic sediments: the LSCE benthic station	
Autores: 	Toussaint, Flora; Rabouille, Christophe; Cathalot, Cecile; Bombled, Bruno; Abchiche, Abdel; Aouji, Oualid; Buchholtz, Gilles; Clemencon, Aurelien; Geyskens, Nicolas; Repecaud, Michel; Pairaud, Ivane; Verney, Romaric; Tisnerat-laborde, Nadine.	
Data: 	2014-11	
Ano: 	2014	
Resumo: 	A new benthic station equipped with oxygen microelectrodes and environmental sensors was developed by Laboratoire des Sciences du Climat et de L’Environnement (LSCE) and Division Technique of the Institut National des Sciences de L’Univers (DT-INSU) to perform in situ time series monitoring of sediment oxygen demand, linked to the mineralization of organic matter. The time series typically cover periods of 2-3 months, with a base frequency of 1 set of oxygen profiles per day. The profiling head assessed the lateral heterogeneity of the sediment oxygen demand at the beginning of the time series over a 0.8-m long rectangle to discriminate spatial and temporal variability. A continuous recalibration is performed using a moored oxygen optode anchored to the benthic station together with a set of environmental sensors. These sensors (turbidity, temperature, salinity, and oxygen) can trigger a high-frequency profiling mode to investigate the fate of particulate organic matter delivered during floods, resuspension, and deposition events. Deployments of the benthic station were performed in the Rhone River subaqueous delta (Mediterranean Sea). We show that “stable” periods (when neither floods nor storms occur) were characterized by a stable oxygen demand. In the case of resuspension events, an increase of the sediment oxygen demand by a factor of 2-3 with a relaxation time of 1 day was observed, indicating that the new benthic station can adequately capture the impact of resuspension events on the oxygen demand in deltaic sediments.	
Tipo: 	Text	
Idioma: 	Inglês	
Identificador: 	http://archimer.ifremer.fr/doc/00230/34126/32597.pdf

http://archimer.ifremer.fr/doc/00230/34126/36349.pdf

DOI:10.4319/lom.2014.12.729

http://archimer.ifremer.fr/doc/00230/34126/	
Editor: 	Amer Soc Limnology Oceanography	
Formato: 	application/pdf	
Fonte: 	Limnology And Oceanography-methods (1541-5856) (Amer Soc Limnology Oceanography), 2014-11 , Vol. 12 , P. 729-741	
Fonte: 	2014, by the American Society of Limnology and Oceanography, Inc.

info:eu-repo/semantics/openAccess

restricted use