Data/hora: 06/06/2024 00:38:52

Provedor de dados: | 5
País: | France
Título: | Caractérisation expérimentale et numérique d’hydroliennes : études de deux hydroliennes en interaction
Autores: | Carlier, Clement; Pinon, Gregory; Mycek, Paul; Gaurier, Benoit; Germain, Gregory; Rivoalen, Elie.
Data: | 2014-11
Ano: | 2014
Resumo: | The development of marine current turbines arrays still needs nowadays many studies among which we can find the study of interactions between devices. In order to highlight these interactions effects, experiments were carried out in the IFREMER’s (Boulogne-sur-Mer) flume tank. Those experiments used 3-bladed horizontal axis marine current turbines prototypes, regulated in rotation speed. To complete these experiments, a three-dimensional numerical tool is developed at the LOMC (Université du Havre) to simulate one or more turbines in a free upstream current. We present hereafter the numerical and experimental results obtained in the scope of the study of elementary interaction between two turbines axially aligned with the upstream current.
Tipo: | Text
Idioma: | Francês

Identificador:

http://archimer.ifremer.fr/doc/00247/35806/34320.pdf

http://archimer.ifremer.fr/doc/00247/35806/

Editor: | 14èmes journées de l'Hydrodynamique, Val de Reuil, 18-20 novembre 2014
Formato: | application/pdf

Fonte:

info:eu-repo/semantics/openAccess

restricted use