Data/hora: 07/06/2024 06:48:54

Provedor de dados: 	5	
País: 	France	
Título: 	Fatigue resistance of natural rubber in seawater with comparison to air	
Autores: 	Ulu, K. Narynbek; Huneau, B.; Le Gac, Pierre-yves; Verron, E.	
Data: 	2016-07	
Ano: 	2016	
Palavras-chave: 	Natural rubber; Fatigue; Environmental effects; Seawater; Strain-induced crystallization.	
Resumo: 	Fatigue properties of filled natural rubber in seawater environment are investigated by uniaxial fatigue and crack propagation experiments, and the damage is analyzed by scanning electron microscopy. The behavior under relaxing and non-relaxing loading conditions is studied and the results are compared to those obtained in air environment. For relaxing loading conditions, fatigue behavior is the same in both environments. Under non-relaxing conditions at large strain levels, for which the influence of strain-induced crystallization is important, fatigue life is longer in seawater. Such behavior could be explained by increased internal temperatures of specimens tested in air due to lower heat conductivity of air as compared to seawater. Such conclusion is also supported by the damage mechanisms observed under non-relaxing loading conditions.	
Tipo: 	Text	
Idioma: 	Inglês	
Identificador: 	http://archimer.ifremer.fr/doc/00324/43523/43055.pdf

DOI:10.1016/j.ijfatigue.2016.03.033

http://archimer.ifremer.fr/doc/00324/43523/	
Editor: 	Elsevier Sci Ltd	
Formato: 	application/pdf	
Fonte: 	International Journal Of Fatigue (0142-1123) (Elsevier Sci Ltd), 2016-07 , Vol. 88 , P. 247-256	
Fonte: 	2016 Elsevier Ltd. All rights reserved.

info:eu-repo/semantics/openAccess

restricted use