Data/hora: 11/06/2024 08:11:15

Provedor de dados: 	5	
País: 	France	
Título: 	Influence of Through-Thickness Pinning on Composite Shear Properties	
Autores: 	Maurin, Romain; Baley, Christophe; Cartie, Denis D. R.; Davies, Peter.	
Data: 	2012-12	
Ano: 	2012	
Palavras-chave: 	Z-pinning; Shear; Mode II; Damage; Acoustic emission.	
Resumo: 	This paper describes results from tests to examine the influence of through-thickness pinning on in-plane shear behaviour, measured by tensile loading of +/- 45A degrees specimens. Samples were produced by both aeronautical and marine manufacturing processes. As few previous studies have investigated pinning of marine composites these were also subjected to out-of-plane shear delamination tests. For both carbon/epoxy laminates the pins reduce the apparent in-plane shear modulus and strength. Pins modify the strain field measured by full-field image analysis, and slow damage development. A new damage mechanism, transverse pin cracking, was observed.	
Tipo: 	Text	
Idioma: 	Inglês	
Identificador: 	http://archimer.ifremer.fr/doc/00113/22390/20186.pdf

DOI:10.1007/s10443-011-9196-9	
Editor: 	Springer	
Relação: 	http://archimer.ifremer.fr/doc/00113/22390/	
Formato: 	application/pdf	
Fonte: 	Applied Composite Materials (0929-189X) (Springer), 2012-12 , Vol. 19 , N. 6 , P. 853-864	
Fonte: 	Springer Science+Business Media B.V. 2011