Data/hora: 01/06/2024 08:36:02

Provedor de dados: | 5
País: | France
Título: | Evaluation of Basalt Fibre Composites for Marine Applications
Autores: | Davies, Peter; Verbouwe, W.
Data: | 2018-04
Ano: | 2018
Palavras-chave: | Seawater; Aging; Fatigue; Basalt fibre; Epoxy; Unidirectional; Flexure.
Resumo: | Basalt fibres offer potential for use in marine structures, but few data exist to evaluate the influence of seawater immersion on their mechanical behaviour. This paper provides the results from a study in which basalt fibre reinforced epoxy composites were aged in natural seawater at different temperatures. Tests were performed under quasi-static and cyclic loading, first in the as-received state then after saturation in natural seawater. Results are compared to those for an E-glass reinforced composite with the same epoxy matrix. They indicate similar mechanical performance for both materials after seawater saturation.
Tipo: | Text
Idioma: | Inglês

Identificador:

http://archimer.ifremer.fr/doc/00392/50385/51111.pdf

DOI:10.1007/s10443-017-9619-3

http://archimer.ifremer.fr/doc/00392/50385/

Editor: | Springer
Formato: | application/pdf
Fonte: | Applied Composite Materials (0929-189X) (Springer), 2018-04 , Vol. 25 , N. 2 , P. 299-308

Fonte:

Springer Science+Business Media B.V. 2017

info:eu-repo/semantics/openAccess

restricted use