Data/hora: 05/06/2024 06:32:59

Provedor de dados: 	5	
País: 	France	
Título: 	Deep-Arvor: a CTD &amp; DO profiling float for Argo	
Autores: 	Le Reste, Serge; Dutreuil, Vincent; Andre, Xavier; Trautmann, Coralie; Bescond, Tanguy.	
Data: 	2012-09-26	
Ano: 	2012	
Resumo: 	The first prototype of Deep-Arvor was deployed this summer. Deep-Arvor is designed to achieve more than 150 profiles from 3500 meters depth, with CTD continuously pumping and oxygen measurements. High resolution profiles are transmitted by the Iridium satellite system. Deep-Arvor maintains the self-ballasting feature of Provor/Arvor and the easy deployment of Arvor thanks to its light weight.	
Tipo: 	Text	
Idioma: 	Inglês	
Identificador: 	http://archimer.ifremer.fr/doc/00115/22627/20352.pdf	
Editor: 	Argo Science Workshop, Venise, 26-29 sept 2012	
Relação: 	http://archimer.ifremer.fr/doc/00115/22627/	
Formato: 	application/pdf	
Fonte: 	2012 Ifremer