Data/hora: 07/06/2024 09:28:35

Provedor de dados: | 5
País: | France
Título: | TRANSMER, un modèle hydrodynamique rapide et précis pour la simulation à moyen et long terme des transferts de radionucléides en Manche et dans le sud de la Mer du Nord
Autores: | Bailly Du Bois, Pascal; Dumas, Franck.
Data: | 2004-09
Ano: | 2004
Palavras-chave: | English Channel; North Sea; Radionuclide; Concentration; Dispersion; Dissolved substances; Seawater; Hydrodynamic model; Modèle; Sb 125; Dispersion; Mer du Nord; Manche.
Resumo: | TRANSMER hydrodynamic model simulates dispersion of dissolved substances in seawater at the scale of the English Channel and the south of the North Sea with a mesh size of one kilometre and a time step of 30 minutes. It has been qualitatively and quantitatively validated by 1400 measurement of 125Sb in seawater. This model evaluates the medium- and long-term consequences of releases of soluble pollutants in the marine ecosystem under normal or accidental conditions, at a very low computation cost (it takes less than one hour to simulate one year).
Tipo: | Text
Idioma: | Francês
Identificador: | http://archimer.ifremer.fr/doc/2004/acte-563.pdf
Editor: | VIIIèmes Journées Nationales Génie Civil ¿ Génie Côtier, Compiègne, 7-9 septembre 2004
Relação: | http://archimer.ifremer.fr/doc/00000/563/
Formato: | application/pdf