Data/hora: 07/06/2024 01:03:42

Provedor de dados: 	5	
País: 	France	
Título: 	TRANSMER, un modèle hydrodynamique rapide et précis pour la simulation à moyen et long terme des transferts de radionucléides en Manche et dans le sud de la Mer du Nord	
Autores: 	Bailly Du Bois, Pascal; Dumas, Franck.	
Data: 	2004-09	
Ano: 	2004	
Palavras-chave: 	English Channel; North Sea; Radionuclide; Concentration; Dispersion; Dissolved substances; Seawater; Hydrodynamic model; Modèle; Sb 125; Dispersion; Mer du Nord; Manche.	
Resumo: 	TRANSMER hydrodynamic model simulates dispersion of dissolved substances in seawater at the scale of the English Channel and the south of the North Sea with a mesh size of one kilometre and a time step of 30 minutes. It has been qualitatively and quantitatively validated by 1400 measurement of 125Sb in seawater. This model evaluates the medium- and long-term consequences of releases of soluble pollutants in the marine ecosystem under normal or accidental conditions, at a very low computation cost (it takes less than one hour to simulate one year).	
Tipo: 	Text	
Idioma: 	Francês	
Identificador: 	http://archimer.ifremer.fr/doc/2004/acte-563.pdf	
Editor: 	VIIIèmes Journées Nationales Génie Civil ¿ Génie Côtier, Compiègne, 7-9 septembre 2004	
Relação: 	http://archimer.ifremer.fr/doc/00000/563/	
Formato: 	application/pdf