Data/hora: 01/06/2024 11:28:44

Provedor de dados: 	5	
País: 	France	
Título: 	Validation d’un procédé automatisé d’extraction sur phase solide de glandes digestives de moules pour l’identification et la quantification des dinophysistoxines en LC/ESI/SM2 par piégeage d’ions quadripolaire	
Autores: 	Mondeguer, Florence; Mestres, Gilberte; Rouland, Caroline; Montagu, Monique; Maillols, Hélène.	
Data: 	2003-02	
Ano: 	2003	
Palavras-chave: 	Toxines; Intoxication des coquillages; Dinophysistoxines; Acide okadaïque; Dinophysistoxine-1; Méthode alternative; Extraction sur phase solide; Automatisation; Couplage CLHP/ESI/SM2 par piège d’ions.; Toxins; Shellfish poisoning; Dinophysistoxins; Okadaic acid; Dinophysistoxin-1; Alternative method; Solid phase extraction; Automation; Liquid chromatography coupled ion trap.	
Resumo: 	This report presents a new extraction method of the dinophysistoxins (DTXs), confirmed by quantification using high-performance liquid chromatography coupled to mass spectrometry with an ion trap and electro spray interface (HPLC/ESI/MS2). The method originality consists on the adaptation of DTXs basic extraction procedure (liquid/ liquid) to a solid phase extraction (SPE) via a robotic station: ASPEC XLi The parameters of the automatization procedure were optimized to obtain the best DTXs recovery rate. These improvements were loaded with digestive gland mussel homogenat realized on a silica cartridge SPE, activated in hexane/chloroform (50:50), washed with hexane/chloroform (50:50) and extracted by an elution gradient (chloroform methanol (65:35) and methanol (100%)). This method was validated according to two normative referentials (linearity, detection quantification limits and accuracy…) : - The Guide of the Pharmacy industry: Analytical Validation, report of the commission SFSTP 1992 (French Corporation of the Sciences and Technical Pharmaceutical), - - The Procedure of validation of an alternative method in compare to a reference method. (AFNOR, 1998. NF V 03-110). Comparison with the classical liquid/liquid extraction and the automated method present clear advantages. In an analytical method the extraction is generally considered to be the most labor-intensive and error-prone step. This new procedure allowed us to increase throughput, to improve the reproducibility and to reduce the error risks due to the individual manual treatments.	
Tipo: 	Text	
Idioma: 	Francês	
Identificador: 	http://archimer.ifremer.fr/doc/00342/45270/44724.pdf

http://archimer.ifremer.fr/doc/00342/45270/	
Formato: 	application/pdf	
Fonte: 	2003 Ifremer

info:eu-repo/semantics/openAccess

restricted use