Data/hora: 01/06/2024 10:43:51

Provedor de dados: | 5
País: | France
Título: | Modeling mud transport in a macrotidal estuary
Autores: | Le Hir, Pierre; Bassoullet, Philippe; L'Yavanc, Jacky.
Data: | 1988
Ano: | 1988
Resumo: | In order to determine the fate of the fine particles and adsorbed contaminants in a short macrotidal estuary, a mathematical modelling system for cohesive suspended mater transport and bottom evolution, including a new consolidation algorithm, is developed. An analysis of successive erosion, transport and deposition processes due to tidal forcing is given and comparisons with field data are provided. A description of mean-terrn bottom variations has been attempted and is partially validated by differential sounding.
Tipo: | Text
Idioma: | Francês
Identificador: | http://archimer.ifremer.fr/doc/00080/19146/16741.pdf
Relação: | http://archimer.ifremer.fr/doc/00080/19146/
Formato: | application/pdf