Data/hora: 08/06/2024 10:06:52

Provedor de dados: 	52	
País: 	Brazil	
Título: 	Response surface methodology to evaluation the recovery of amylases by hollow fiber membrane	
Autores: 	Severo Júnior,João Baptista; Oliveira,Laura Sampaio de Sá; Sardeiro,Fernanda Silva; Souza,Roberto Rodrigues de; Lopes,Francisco Luiz Gumes; Santana,José Carlos Curvelo; Tambourgi,Elias Basile.	
Data: 	2007-07-01	
Ano: 	2007	
Palavras-chave: 	Hollow fiber membrane; Corn malt; Alpha and beta amylase; RSM.	
Resumo: 	This work aimed to study the pH and the transmembrane pressure effects during the recovery of alpha and beta amylases enzymes from corn malt (Zea mays) by hollow fiber membrane. The optimal condition was obtained for a statistical model, established by response surface methodology (RSM). The response surface analysis showed that the best operation condition for amylolitics enzymes recovery by hollow fiber membrane was 0.05 bar and pH 5.00, while the enzymes were purified about of 26 times.	
Tipo: 	Info:eu-repo/semantics/article	
Idioma: 	Inglês	
Identificador: 	http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1516-89132007000400017	
Editor: 	Instituto de Tecnologia do Paraná - Tecpar	
Relação: 	10.1590/S1516-89132007000400017	
Formato: 	text/html	
Fonte: 	Brazilian Archives of Biology and Technology  v.50 n.4 2007	
Fonte: 	info:eu-repo/semantics/openAccess