Data/hora: 06/06/2024 00:21:37

Provedor de dados: 	52	
País: 	Brazil	
Título: 	Dissolved Organic Carbon Determination Using FIA and Photo-Fenton Reaction	
Autores: 	Kondo,Márcia M.; Arcos,Maria A. S. V.; Grassi,Marco T.	
Data: 	2002-03-01	
Ano: 	2002	
Palavras-chave: 	Photo-Fenton reaction; Dissolved organic carbon; FIA.	
Resumo: 	The FIA-photo-Fenton system is based on the flow oxidation of the organic matter. A small amount of the sample containing H2O2 is injected into the acidic flow solution of Fe2+, which passes through a tubular PTFE reactor irradiated with UV light. The generated CO2 is quantified by a conductometric detector and is directly proportional to the dissolved organic carbon concentration in the sample. The optimization studies were performed using EDTA solutions. The average recovery of organic carbon was 83% with a relative standard deviation of 3.7% using a 1:5 molar ratio of Fe2+:H2O2, pH 2.0, 100 muL of sample injection and a liquid flow of 1 mL min-1. After optimization, the DOC concentration was quantified using 13 different organic compounds, where the average recovery was 90%. The rate of the analysis was in average 50 samples hour-1.	
Tipo: 	Info:eu-repo/semantics/article	
Idioma: 	Inglês	
Identificador: 	http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1516-89132002000100013	
Editor: 	Instituto de Tecnologia do Paraná - Tecpar	
Relação: 	10.1590/S1516-89132002000100013	
Formato: 	text/html	
Fonte: 	Brazilian Archives of Biology and Technology  v.45 n.1 2002	
Fonte: 	info:eu-repo/semantics/openAccess