Data/hora: 05/06/2024 08:20:28

Provedor de dados: 	52	
País: 	Brazil	
Título: 	Tratamento biológico de efluentes de indústrias de papel após floculação e coagulação com sais de alumínio e polieletrólitos naturais	
Autores: 	Reis,Edson M. dos; Nozaki,Jorge.	
Data: 	2000-01-01	
Ano: 	2000	
Palavras-chave: 	Flocculation; Natural polyelectrolytes; Biological degradation; Activated sludge process; Paper and pulp effluents.	
Resumo: 	The flocculation and sedimentation of recalcitrant organic compounds of high molecular weight using natural polyelectrolytes, extracted from the cactus Cereus peruvianus and Opuntia ficus indica, have been studied. Organic compounds of high molecular weight from effluents of paper and pulp industries are difficult for biological degradation. However, using a mixture of aluminum salts and natural polyelectrolytes, the aggregation and settling properties of recalcitrant organics were increased if compared with conventional methods of wastewater treatment using only aluminum or iron sulfate. After flocculation, sedimentation, and filtration, the effluent was submitted to biological degradation by activated sludge process. The main advantages of using a mixture of aluminum salts and natural polyelectrolytes were shorter time of flocculation, floccus of larger size and easier for filtration.The removal efficiency observed were:85-90% of aromatic compounds, 70-85% of chemical oxygen demand,and 91-97% of colour.	
Tipo: 	Info:eu-repo/semantics/article	
Idioma: 	Português	
Identificador: 	http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1516-89132000000100016	
Editor: 	Instituto de Tecnologia do Paraná - Tecpar	
Relação: 	10.1590/S1516-89132000000100016	
Formato: 	text/html	
Fonte: 	Brazilian Archives of Biology and Technology  v.43 n.1 2000	
Fonte: 	info:eu-repo/semantics/openAccess