Data/hora: 01/06/2024 07:35:00

Provedor de dados: 	52	
País: 	Brazil	
Título: 	Performance of the constructed wetland system for the treatment of water from the corumbataí river	
Autores: 	Borges,Ana Kleiber Pessoa; Tauk-Tornisielo,Sâmia Maria; Domingos,Roberto Naves; Angelis,Dejanira de Franceschi de.	
Data: 	2008-12-01	
Ano: 	2008	
Palavras-chave: 	Aquatic macrophytes; Filtering soil; Microfiltration; Bioreactor; Microorganisms.	
Resumo: 	The aim of this work was to study the constructed wetland system for the treatment of water from the Corumbataí river simulated on a laboratory scale. The parameters analyzed at different points of the system were ammonia, biochemical demand for oxygen (BDO), chemical demand for oxygen (CDO), chlorides, apparent color, conductivity, dissolved oxygen, magnesium (Mg), sodium (Na), potassium (K), silicon (Si), total phosphorous, total coliforms and Escherichia coli, total dissolved solids (TDS), turbidity, and macrophyte biomass. The results demonstrated that this alternative water treatment system was effective in removing the microorganisms (total coliforms and E. coli), among other parameters analyzed, for varying periods of the treatment, promoting notable improvement in the quality of the water treated from the Corumbataí River.	
Tipo: 	Info:eu-repo/semantics/article	
Idioma: 	Inglês	
Identificador: 	http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1516-89132008000600024	
Editor: 	Instituto de Tecnologia do Paraná - Tecpar	
Relação: 	10.1590/S1516-89132008000600024	
Formato: 	text/html	
Fonte: 	Brazilian Archives of Biology and Technology  v.51 n.6 2008	
Fonte: 	info:eu-repo/semantics/openAccess