Data/hora: 06/06/2024 03:31:12

Provedor de dados: 	63	
País: 	Brazil	
Título: 	Soil spatial variability and the estimation of the irrigation water depth	
Autores: 	Reichardt,Klaus; Silva,José Carlos de Araújo; Bassoi,Luis Henrique; Timm,Luís Carlos; Oliveira,Julio Cesar Martins de; Bacchi,Osny Oliveira Santos; Pilotto,João Eduardo.	
Data: 	2001-09-01	
Ano: 	2001	
Palavras-chave: 	Irrigation water depth; Field capacity; Spatial variability.	
Resumo: 	The effects of soil water spatial variability previous to irrigation and of the field capacity on the estimation of irrigation water depth are evaluated. The experiment consisted of a common bean (Phaseolus vulgaris L.) crop established on a Kandiudalfic Eutrudox of Piracicaba, SP, Brazil, irrigated by central pivot, in which soil water contents were evaluated with a depth neutron gauge, in a grid of 20x4 points with lag of 0.5 m. In a given situation, the 80 calculated irrigation water depths presented a coefficient of variation of 29.3%, with an average water value of 18 mm, maximum of 41mm and minimum of 9 mm. It is concluded that the only practical way of irrigation is the use of an average water depth, due to the inherent variability of the soil, and that the search for better field capacity values does not imply in better water depth estimates.	
Tipo: 	Info:eu-repo/semantics/article	
Idioma: 	Inglês	
Identificador: 	http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0103-90162001000300017	
Editor: 	São Paulo - Escola Superior de Agricultura "Luiz de Queiroz"	
Relação: 	10.1590/S0103-90162001000300017	
Formato: 	text/html	
Fonte: 	Scientia Agricola  v.58 n.3 2001	
Fonte: 	info:eu-repo/semantics/openAccess