Data/hora: 10/06/2024 11:20:32

Provedor de dados: 	63	
País: 	Brazil	
Título: 	Cassava processing wastewater as a platform for third generation biodiesel production	
Autores: 	Neves,Cristina; Maroneze,Mariana Manzoni; Santos,Aline Meireles dos; Francisco,Erika Cristina; Wagner,Roger; Zepka,Leila Queiroz; Jacob-Lopes,Eduardo.	
Data: 	2016-10-01	
Ano: 	2016	
Palavras-chave: 	Microalgae; Cyanobacteria; Agroindustrial wastewater; Biofuel.	
Resumo: 	ABSTRACT This study aimed to evaluate third generation biodiesel production by microalgae Phormidium autumnale using cassava processing wastewater as a platform. Experiments were performed in a heterotrophic bubble column bioreactor. The study focused on the evaluation of the bioreactor (batch and fed-batch) of different operational modes and the analysis of biofuel quality. Results indicate that fed-batch cultivations improved system performance, elevating biomass and oil productions to 12.0 g L−1 and 1.19 g L−1, respectively. The composition of this oil is predominantly saturated (60 %) and monounsaturated (39 %), resulting in a biodiesel that complys with U.S., European and Brazilian standards. The technological route developed indicates potential for sustainable production of bulk oil and biodiesel, through the minimization of water and chemical demands required to support such a process.	
Tipo: 	Info:eu-repo/semantics/article	
Idioma: 	Inglês	
Identificador: 	http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0103-90162016000500412	
Editor: 	São Paulo - Escola Superior de Agricultura "Luiz de Queiroz"	
Relação: 	10.1590/0103-9016-2015-0302	
Formato: 	text/html	
Fonte: 	Scientia Agricola  v.73 n.5 2016	
Fonte: 	info:eu-repo/semantics/openAccess