Data/hora: 02/06/2024 18:58:22

Provedor de dados: 	65	
País: 	Brazil	
Título: 	Embedded system in Arduino platform with Fuzzy control to support the grain aeration decision	
Autores: 	Szesz Junior,Albino; Monteiro Junior,Marcos; Dias,Ariangelo Hauer; Mathias,Ivo Mário; Conti,Giuvane.	
Data: 	2016-11-01	
Ano: 	2016	
Palavras-chave: 	Arduino; Agriculture; Mathematical model; Fuzzy logic; Grain aeration.	
Resumo: 	ABSTRACT: Aeration is currently the most commonly used technique to improve the drying and storage of grain, depending on temperature and water content of the grain, as of the temperature and relative humidity of the outside air. In order to monitor temperature and humidity of the grain mass, it is possible to have a network of sensors in the cells of both internal and external storage. Use of artificial intelligence through Fuzzy theory, has been used since the 60s and enables their application on various forms. Thus, it is observed that the aeration of grain in function of representing a system of controlled environment can be studied in relation to the application of this theory. Therefore, the aim of this paper is to present an embedded Fuzzy control system based on the mathematical model of CRUZ et al. (2002) and applied to the Arduino platform, for decision support in aeration of grain. For this, an embedded Arduino system was developed, which received the environmental values of temperature and humidity to then be processed in a Fuzzy controller and return the output as a recommendation to control the aeration process rationally. Comparing the results obtained from the graph presented by LASSERAN (1981) it was observed that the system is effective.	
Tipo: 	Info:eu-repo/semantics/article	
Idioma: 	Inglês	
Identificador: 	http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0103-84782016001101917	
Editor: 	Universidade Federal de Santa Maria	
Relação: 	10.1590/0103-8478cr20141808	
Formato: 	text/html	
Fonte: 	Ciência Rural  v.46 n.11 2016	
Fonte: 	info:eu-repo/semantics/openAccess