Data/hora: 12/06/2024 07:51:28

Provedor de dados: 	70	
País: 	Brazil	
Título: 	Energetic efficiency of a deep bed swine production system	
Autores: 	Veloso,Alessandro V.; Campos,Alessandro T.; Paula,Vanderson R. de; Dourado,David C.; Yanagi Júnior,Tadayuki; Silva,Enilson B.	
Data: 	2012-12-01	
Ano: 	2012	
Palavras-chave: 	Energy input and output; Swine buildings; Alternative management; Sustainability of biosystems.	
Resumo: 	The aim of this work was to evaluate the energy flows of a commercial production system of swine deep bed in its finishing phase, located in Juiz de Fora, in the State of Minas Gerais, Brazil. Thus, an energy efficiency study was carried out by monitoring a lot of animals, during a 94-day period. The energy rate of each compound involved in the production process was quantified and the matrixes of energy consumption were determined in the form of animal feeding, electrical energy, piglets, material used as deep bed, human labor, equipment, swine buildings, production of alive swine for slaughter, organic fertilizer production (swine deep bed or swine deep litter). From the direct input energy, 80.57% correspond to animal feeding, 11.90% to pigs for slaughter and 6.76% to piglets, while from the energy output 53.45% correspond to the terminating swine and 46.55% to organic fertilizer (swine deep bed). By the results obtained, we can conclude that such production system has corresponded to an industrial and highly specialized agro ecosystem, importing a great part of the energy consumed in the production process, with 41% of energy efficiency.	
Tipo: 	Info:eu-repo/semantics/article	
Idioma: 	Inglês	
Identificador: 	http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000600008	
Editor: 	Associação Brasileira de Engenharia Agrícola	
Relação: 	10.1590/S0100-69162012000600008	
Formato: 	text/html	
Fonte: 	Engenharia Agrícola  v.32 n.6 2012	
Fonte: 	info:eu-repo/semantics/openAccess