Data/hora: 02/06/2024 19:10:39

Provedor de dados: | 70
País: | Brazil
Título: | Estimation of transpiration of the 'Valencia' orange young plant using thermal dissipation probe method
Autores: | Coelho,Rubens D.; Vellame,Lucas M.; Fraga Júnior,Eusímio F.
Data: | 2012-06-01
Ano: | 2012
Palavras-chave: | Lysimetry; Sap flow; Xylem.
Resumo: | Most studies on measures of transpiration of plants, especially woody fruit, relies on methods of heat supply in the trunk. This study aimed to calibrate the Thermal Dissipation Probe Method (TDP) to estimate the transpiration, study the effects of natural thermal gradients and determine the relation between outside diameter and area of xylem in 'Valencia' orange young plants. TDP were installed in 40 orange plants of 15 months old, planted in boxes of 500 L, in a greenhouse. It was tested the correction of the natural thermal differences (DTN) for the estimation based on two unheated probes. The area of the conductive section was related to the outside diameter of the stem by means of polynomial regression. The equation for estimation of sap flow was calibrated having as standard lysimeter measures of a representative plant. The angular coefficient of the equation for estimating sap flow was adjusted by minimizing the absolute deviation between the sap flow and daily transpiration measured by lysimeter. Based on these results, it was concluded that the method of TDP, adjusting the original calibration and correction of the DTN, was effective in transpiration assessment.
Tipo: | Info:eu-repo/semantics/article
Idioma: | Inglês
Identificador: | http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000300016
Editor: | Associação Brasileira de Engenharia Agrícola
Relação: | 10.1590/S0100-69162012000300016
Formato: | text/html
Fonte: | Engenharia Agrícola  v.32 n.3 2012
Fonte: | info:eu-repo/semantics/openAccess