Data/hora: 12/06/2024 04:21:33

Provedor de dados: | 70
País: | Brazil
Título: | Method of numerical correction of errors occasioned by delay of records during the monitoring of environmental variables of interest for animal production
Autores: | Gabriel Filho,Luís R. A.; Pereira,Danilo F.; Barato,Fernando F.; De Magalhães,Marcelo M.
Data: | 2011-10-01
Ano: | 2011
Palavras-chave: | Geoestatistical; Animal precision production; Mathematical methods.
Resumo: | Thermal and air conditions inside animal facilities change during the day due to the influence of the external environment. For statistical and geostatistical analyses to be representative, a large number of points spatially distributed in the facility area must be monitored. This work suggests that the time variation of environmental variables of interest for animal production, monitored within animal facility, can be modeled accurately from discrete-time records. The aim of this study was to develop a numerical method to correct the temporal variations of these environmental variables, transforming the data so that such observations are independent of the time spent during the measurement. The proposed method approached values recorded with time delays to those expected at the exact moment of interest, if the data were measured simultaneously at the moment at all points distributed spatially. The correction model for numerical environmental variables was validated for environmental air temperature parameter, and the values corrected by the method did not differ by Tukey's test at 5% significance of real values recorded by data loggers.
Tipo: | Info:eu-repo/semantics/article
Idioma: | Inglês
Identificador: | http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000500001
Editor: | Associação Brasileira de Engenharia Agrícola
Relação: | 10.1590/S0100-69162011000500001
Formato: | text/html
Fonte: | Engenharia Agrícola  v.31 n.5 2011
Fonte: | info:eu-repo/semantics/openAccess