Data/hora: 12/06/2024 14:19:21

Provedor de dados: | 70
País: | Brazil
Título: | CORN FERTILIZATION USING SWINE WASTEWATER AND SOIL-WATER ENVIRONMENTAL QUALITY
Autores: | Rosa,Danielle M.; Sampaio,Silvio C.; Pereira,Pâmela A. M.; Reis,Ralpho R. Dos; Sbizzaro,Mariana.
Data: | 2017-08-01
Ano: | 2017
Palavras-chave: | Liquid residue of swine; No-tillage; Water reuse.
Resumo: | ABSTRACT: Soil application of swine wastewater for nutrient cycling may represent a correct destination of these residues and reduction in production costs. However, when applied to soil, such residue may cause environmental impacts. This study aimed to analyze the chemical characteristics of the soil, corn, and leachate after successive swine wastewater applications associated with mineral fertilization. The experiment was developed in drainage lysimeters under field conditions. Wastewater doses applied were 0, 100, 200, and 300 m3 ha−1 with and without mineral fertilization. The results were submitted to analysis of variance and Tukey's test. After nine years of application, a special attention should be taken regarding water quality from a dose of 200 m3 ha−1 since some elements may leach into the soil. In addition, a synchronism between residue application and crop requirements needs to be taken into account. Doses of 200 and 300 m3 ha−1 are considered as satisfactory to meet corn nutritional requirements. Moreover, an increase in fertility characteristics was observed, but a caution regarding Cu and Zn contents should be taken since these elements produce a cumulative effect in the soil.
Tipo: | Info:eu-repo/semantics/article
Idioma: | Inglês
Identificador: | http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000400801
Editor: | Associação Brasileira de Engenharia Agrícola
Relação: | 10.1590/1809-4430-eng.agric.v37n4p801-810/2017
Formato: | text/html
Fonte: | Engenharia Agrícola  v.37 n.4 2017
Fonte: | info:eu-repo/semantics/openAccess