Data/hora: 06/06/2024 02:45:09

Provedor de dados: 	70	
País: 	Brazil	
Título: 	Effect of a simulated heat wave in thermal and aerial environment broiler-rearing environment	
Autores: 	Vale,Marcos M. do; Moura,Daniella J. de; Nääs,Irenilza de A.; Curi,Thayla M. R. C.; Lima,Karla A. O.	
Data: 	2016-04-01	
Ano: 	2016	
Palavras-chave: 	Ammonia; Gas production; Animal welfare; Oxygen; Litter temperature.	
Resumo: 	ABSTRACT Global warming increases the occurrence of events such as extreme heat waves. Research on thermal and air conditions affecting broiler-rearing environment are important to evaluate the animal welfare under extreme heat aiming mitigation measures. This study aimed at evaluating the effect of a simulated heat wave, in a climatic chamber, on the thermal and air environment of 42-day-old broilers. One hundred and sixty broilers were housed and reared for 42 days in a climatic chamber; the animals were divided into eight pens. Heat wave simulation was performed on the 42nd day, the period of great impact and data sampling. The analyzed variables were room and litter temperatures, relative humidity, concentrations of oxygen, carbon monoxide and ammonia at each pen. These variables were assessed each two hours, starting at 8 am, simulating a day heating up to 4 pm, when it is reached the maximum temperature. By the results, we concluded that increasing room temperatures promoted a proportional raise in litter temperatures, contributing to ammonia volatilization. In addition, oxygen concentrations decreased with increasing temperatures; and the carbon monoxide was only observed at temperatures above 27.0 °C, relative humidity higher than 88.4% and litter temperatures superior to 30.3 °C.	
Tipo: 	Info:eu-repo/semantics/article	
Idioma: 	Inglês	
Identificador: 	http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000200271	
Editor: 	Associação Brasileira de Engenharia Agrícola	
Relação: 	10.1590/1809-4430-Eng.Agric.v36n2p271-280/2016	
Formato: 	text/html	
Fonte: 	Engenharia Agrícola  v.36 n.2 2016	
Fonte: 	info:eu-repo/semantics/openAccess