Data/hora: 02/06/2024 18:21:18

Provedor de dados: 	70	
País: 	Brazil	
Título: 	Poultry carcass decomposition and physicochemical analysis of compounds in different Composter types	
Autores: 	Cestonaro,Taiana; Abreu,Paulo G. de; Abreu,Valéria M. N.; Lopes,Letícia dos S.; Coldebella,Arlei.	
Data: 	2014-08-01	
Ano: 	2014	
Palavras-chave: 	Composting; Organic fertilizers; Substrate.	
Resumo: 	This study aimed to assess five composter types in poultry carcasses decomposition and to perform a physicochemical analysis of the compounds obtained. Composter types used were six-hole brick, wood, screen, windrow with three PVC pipes with six holes and windrow with three PVC pipes with 10 holes. Composting was followed by four periods using wood shaving like substrate with one bird carcass placed in each composter. Pile turning was performed every 10 days and temperature in each layer was measured on 1st, 7th, 14th, 19th and 29th day, at 3 p.m., as well as room temperature. Temperature during pile turning was also measured at five points per layer and carcass weighing performed to calculate decomposition percentage. Physicochemical parameters evaluated in substrates were moisture, ash, phosphorus, potassium, nitrogen, pH, organic carbon and C/N ratio, up to 30 days. Data were analyzed by repeated measures model, using MIXED method of SAS software. All values of final physicochemical composition of substrates were found according to values of IN-25, except nitrogen. The composter types were efficient in decomposition of poultry carcasses.	
Tipo: 	Info:eu-repo/semantics/article	
Idioma: 	Inglês	
Identificador: 	http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000400002	
Editor: 	Associação Brasileira de Engenharia Agrícola	
Relação: 	10.1590/S0100-69162014000400002	
Formato: 	text/html	
Fonte: 	Engenharia Agrícola  v.34 n.4 2014	
Fonte: 	info:eu-repo/semantics/openAccess