Data/hora: 03/06/2024 07:49:29

Provedor de dados: | 70
País: | Brazil
Título: | Automatic and manual spray bar sections control
Autores: | Weirich Neto,Pedro H.; Meer,Roderik W. V. D.; Vink,Peter; Justino,Altair; Garcia,Luiz C.
Data: | 2014-12-01
Ano: | 2014
Palavras-chave: | Precision farming and pesticide application technology.
Resumo: | The use of precision farming tools in pesticide application technology can improve the techniques effectiveness during the spraying. Thus, this study aimed to compare automatic and manual systems to interrupt the syrup flow in the spray bar sections when applied in overlapped areas. The sprayings were carried out in eight places in completely randomized design. It was compared the spray consumption and the sprayed area in relation to the total area. The results indicated that in sprays performed with the automatic system there was an average savings of 17.2% of the sprayed volume. The sprayed area using the bar section's automatic control was an average 6.1% lower than the sprayed area with manual control.
Tipo: | Info:eu-repo/semantics/other
Idioma: | Inglês
Identificador: | http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000600015
Editor: | Associação Brasileira de Engenharia Agrícola
Relação: | 10.1590/S0100-69162014000600015
Formato: | text/html
Fonte: | Engenharia Agrícola  v.34 n.6 2014
Fonte: | info:eu-repo/semantics/openAccess