Data/hora: 05/06/2024 01:35:36

Provedor de dados: | 70
País: | Brazil
Título: | Distribution of water in sandy soil applied by drip
Autores: | Gonçalves,Antônio C. A.; Alves,Daniel S.; Marques,Patricia A. A.; Folegatti,Marcos V.; José,Jefferson V.
Data: | 2014-12-01
Ano: | 2014
Palavras-chave: | Time Domain Reflectometry; TDR probes; Irrigation.
Resumo: | The search for the use of water with high levels of efficiency has motivated the use of drip irrigation in several agricultural systems. However, for the efficiency be ensured, it is necessary that the water distribution in the soil profile must to be known in more details. As it is a highly variable process, function of the local characteristics, is essential the study of each case. The objective of this research was evaluating the water distribution in the soil profile, from drippers installed in surface and 0.15 m below the soil surface. The experiment was realized in the Technical Center of Irrigation (TCI) of the State University of Maringá - PR. The water monitoring in the soil profile was done with TDR probes installed in a box containing sandy soil, at the depths from 0.05 to 0.80 m; and 0.05 to 0.35 m of lateral spacing, at intervals of 0.05 m, totalizing 30 probes. The treatments were differentiated in relation of the installation depth of the emitters (0.0 and 0.15 m) and flow (1, 2, 4, 6, and 8 L h-1). The irrigation time was 8 hours continuous with reading of the TDR probes each 30 minutes. The results allowed concluding that the wet area with the emitter positioned on the soil surface was directly proportional to the flow increase. For the underground dripper, this area was substantially smaller and the water losses by percolation were higher, mainly to the flows higher than 4 L h-1, which provided to unacceptable water losses that should be avoided.
Tipo: | Info:eu-repo/semantics/other
Idioma: | Inglês
Identificador: | http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000600013
Editor: | Associação Brasileira de Engenharia Agrícola
Relação: | 10.1590/S0100-69162014000600013
Formato: | text/html
Fonte: | Engenharia Agrícola  v.34 n.6 2014
Fonte: | info:eu-repo/semantics/openAccess