Data/hora: 14/06/2024 09:49:18

Provedor de dados: 	83	
País: 	Brazil	
Título: 	Design and construction of an Electric Fish Finder	
Autores: 	Crampton,William G. R.; Wells,Jonathan K.; Smyth,Charles; Walz,Steven A.	
Data: 	2007-09-01	
Ano: 	2007	
Palavras-chave: 	Electric Organ Discharge; Gymnotiformes; Knifefishes; Method.	
Resumo: 	We provide notes on the design and construction of an Electric Fish Finder - a portable differential amplifier for detecting the electrostatic fields of gymnotiform knifefishes. The device can be adapted to locate electric fishes in any kind of aquatic environment. It is rugged, water resistant, and powered by alkaline batteries. This contribution is part of a series of technical papers designed to encourage students of neotropical ichthyology to explore the ecology, systematics, and electric signaling of gymnotiform fishes.	
Tipo: 	Info:eu-repo/semantics/article	
Idioma: 	Inglês	
Identificador: 	http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1679-62252007000300022	
Editor: 	Sociedade Brasileira de Ictiologia	
Relação: 	10.1590/S1679-62252007000300022	
Formato: 	text/html	
Fonte: 	Neotropical Ichthyology  v.5 n.3 2007	
Fonte: 	info:eu-repo/semantics/openAccess