Consulta: creatorFacets:"Burks, Thomas F."
Registros recuperados: 3
Data/hora: 06/06/2024 01:11:38

Citrus black spot detection using hyperspectral image analysis
Provedor de dados: 111
Autores: Bulanon, Duke M.; Burks, Thomas F.; Kim, Dae G.; Ritenour, Mark A.
A recently discovered fungal disease called citrus black spot, is threatening the Florida citrus industry.  The fungal disease, which causes cosmetic lesions on the rind of the fruit and can cause a tree to drop its fruit prematurely, could possibly lead to a ban on sales of fresh Florida citrus in other citrus-producing states.  The objective of this research is to develop a multispectral imaging algorithm to detect citrus black spots based on hyperspectral image data.  Hyperspectral images of citrus fruits (Valencias) were collected in the wavelength range of 480 nm to 950 nm.  Five surface conditions were examined, citrus black spot, greasy spot, melanose, wind scar, and normal one.  The first part of the image analysis determined the optimal...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Agricultural Engineering citrus disease; Multispectral imaging; Hyperspectral imaging.
Ano: 2013
URL: http://www.cigrjournal.org/index.php/Ejounral/article/view/2382

Edge effect compensation for citrus canker lesion detection due to light source variation – a hyperspectral imaging application
Provedor de dados: 111
Autores: Niphadkar, Nikhil P.; Burks, Thomas F.; Qin, Jianwei; Ritenour, Mark.
The spread of citrus canker has become one of the most important challenges faced by Florida Fresh Market citrus is affecting the export of citrus fruits to several international markets including European countries.  Previous studies have shown that automated detection systems can help detect citrus canker infected fruit and could assist in eliminating the detected fruit from shipment to closed markets.  Most automated detection systems use some form of machine vision with artificial light sources.  However, when capturing images of spherical objects, non-uniform illumination results in an edge blackening effect resulting in higher misclassification rate.  The basic objective of this research was to implement a compensation algorithm to eliminate the edge...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Edge effect compensation; Hyperspectral imaging; Canker; Spatial correction; Geometric correction.
Ano: 2013
URL: http://www.cigrjournal.org/index.php/Ejounral/article/view/2278

3D Dense Reconstruction of Plant or Tree Canopy Based on Stereo Vision
Provedor de dados: 111
Autores: Ni, Zhijiang; Burks, Thomas F.
Three dimensional (3D) reconstruction of the plant or tree canopy is an important step in order to measure canopy geometry, such as, height, width, volume, and leaf cover area. In this research, binocular stereo vision was used to recover the 3D information of the canopy. A revised camera calibration method was provided to calibrate the cameras in world coordinate system. Only two images were used to realize a dense reconstruction. These two images were firstly rectified to make sure the corresponding feature points in the left and right images were on the same horizontal line. An efficient large scale stereo matching (ELAS) algorithm was used to find the disparity map. The plant or tree canopy was finally reconstructed based on these calibrated camera...
Tipo: Info:eu-repo/semantics/article
Ano: 2018
URL: http://www.cigrjournal.org/index.php/Ejounral/article/view/4358