Consulta: creatorFacets:"Conti,Giuvane"
Registros recuperados: 1
Data/hora: 12/06/2024 00:47:02

Embedded system in Arduino platform with Fuzzy control to support the grain aeration decision
Provedor de dados: 65
Autores: Szesz Junior,Albino; Monteiro Junior,Marcos; Dias,Ariangelo Hauer; Mathias,Ivo Mário; Conti,Giuvane.
ABSTRACT: Aeration is currently the most commonly used technique to improve the drying and storage of grain, depending on temperature and water content of the grain, as of the temperature and relative humidity of the outside air. In order to monitor temperature and humidity of the grain mass, it is possible to have a network of sensors in the cells of both internal and external storage. Use of artificial intelligence through Fuzzy theory, has been used since the 60s and enables their application on various forms. Thus, it is observed that the aeration of grain in function of representing a system of controlled environment can be studied in relation to the application of this theory. Therefore, the aim of this paper is to present an embedded Fuzzy control...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Arduino; Agriculture; Mathematical model; Fuzzy logic; Grain aeration.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0103-84782016001101917