Consulta: creatorFacets:"Hamon, Michel"
Registros recuperados: 8
Data/hora: 01/06/2024 13:37:50

A flow-through rearing system for ecophysiological studies of Pacific oyster Crassostrea gigas larvae
Provedor de dados: 5
Autores: Rico Villa, Benjamin; Woerther, Patrice; Mingant, Christian; Le Piver, David; Pouvreau, Stephane; Hamon, Michel; Robert, Rene.
While literature is relatively abundant on adult shellfish, ecophysiological studies at the larval stage are scarce because of both technical difficulties and inadequate methodology. A tool dedicated to provide basic information for larval ecophysiology was accordingly developed. Two steps were followed: first a flow-through method of Crassostrea gigas larval culture was perfected during a set of experiments in which rearing systems and larval density were assessed. Then a continuous hydrobiological data recorder was adapted with modifications to comply with our experimental aim. SILO (Système d'Instrumentation des Larves en flux Ouvert) allowed the successive acquisition of hydrobiological parameters in ten 150 l larval tanks in which larvae were reared...
Tipo: Text
Palavras-chave: Temperature; Ecophysiology; Bivalve larvae; Crassostrea gigas; Flow through.
Ano: 2008
URL: http://archimer.ifremer.fr/doc/2008/publication-4167.pdf

Introduction to the French GEOTRACES North Atlantic Transect (GA01): GEOVIDE cruise
Provedor de dados: 5
Autores: Sarthou, Geraldine; Lherminier, Pascale; Achterberg, Eric P.; Alonso-perez, Fernando; Bucciarelli, Eva; Boutorh, Julia; Bouvier, Vincent; Boyle, Edward A.; Branellec, Pierre; Carracedo, Lidia I.; Casacuberta, Nuria; Castrillejo, Maxi; Cheize, Marie; Pereira, Leonardo Contreira; Cossa, Daniel; Daniault, Nathalie; De Saint-leger, Emmanuel; Dehairs, Frank; Deng, Feifei; De Gesincourt, Floriane Desprez; Devesa, Jeremy; Foliot, Lorna; Fonseca-batista, Debany; Gallinari, Morgane; Garcia-ibanez, Maribel I.; Gourain, Arthur; Grossteffan, Emilie; Hamon, Michel; Heimburger, Lars Eric; Henderson, Gideon M.; Jeandel, Catherine; Kermabon, Catherine; Lacan, Francois; Le Bot, Philippe; Le Goff, Manon; Le Roy, Emilie; Lefebvre, Alison; Leizour, Stephane; Lemaitre, Nolwenn; Masque, Pere; Menage, Olivier; Barraqueta, Jan-lukas Menzel; Mercier, Herle; Perault, Fabien; Perez, Fiz F; Planquette, Helene; Planchon, Frederic; Roukaerts, Arnout; Sanial, Virginie; Sauzede, Raphaelle; Schmechtig, Catherine; Shelley, Rachel U.; Stewart, Gillian; Sutton, Jill; Tang, Yi; Tisnerat-laborde, Nadine; Tonnard, Manon; Treguer, Paul; Van Beek, Pieter; Zurbrick, Cheryl M.; Zunino Rodriguez, Patricia.
The GEOVIDE cruise, a collaborative project within the framework of the international GEOTRACES programme, was conducted along the French-led section in the North Atlantic Ocean (Section GA01), between 15 May and 30 June 2014. In this special issue (https://www.biogeosciences.net/special_ issue900.html), results from GEOVIDE, including physical oceanography and trace element and isotope cyclings, are presented among 18 articles. Here, the scientific context, project objectives, and scientific strategy of GEOVIDE are provided, along with an overview of the main results from the articles published in the special issue.
Tipo: Text
Ano: 2018
URL: https://archimer.ifremer.fr/doc/00470/58178/60685.pdf

New instruments to monitor coastal sea water masses according to European Water Framework Directive, Trophimatique project
Provedor de dados: 5
Autores: Repecaud, Michel; Degres, Yves; Bernard, Nathalie; Allenou, Jean-pierre; Aoustin, Yannick; Arrondeau, Jean-pierre; Bouget, Jean-francois; Bucas, Karenn; Daniel, Anne; Guillaud, Jean-francois; Hamon, Michel; Jegou, Paul; Laes, Agathe; Le Roux, Dominique; Le Piver, David; Quemener, Loic; Rolin, Jean-francois; Rudelle, Tiphaine; Legrand, Jacques; Vuillemin, Renaud.
The automated monitoring of physico-chemical parameters in the coastal zone has been using large buoys and fixed infrastructures. A better understanding of many estuaries is needed in order to fulfil the agenda and requirements of the European Water Framework Directive. In order to address the fluxes of nutrients as well as algal blooms and low oxygen events, the "TROPHIMATIQUE" project has developed a new generation of instruments able to be deployed in sea waters. The smaller size of the new instruments is intended to facilitate the maintenance. A new multi-parameter probe has been developed. The measurements of all nutrients are performed thanks to the CHEMINI flow injection analysers for nitrate, ammonia, silicate and phosphate. A sampler using similar...
Tipo: Text
Ano: 2009
URL: http://archimer.ifremer.fr/doc/00107/21807/20276.pdf

The CORA dataset: validation and diagnostics of in-situ ocean temperature and salinity measurements
Provedor de dados: 5
Autores: Cabanes, Cecile; Grouazel, Antoine; Von Schuckmann, Karina; Hamon, Michel; Turpin, Victor; Coatanoan, Christine; Paris, Francois; Guinehut, Stephanie; Boone, C.; Ferry, N.; De Boyer Montegut, Clement; Carval, Thierry; Reverdin, Gilles; Pouliquen, Sylvie; Le Traon, Pierre-yves.
The French program Coriolis, as part of the French operational oceanographic system, produces the COriolis dataset for Re-Analysis (CORA) on a yearly basis. This dataset contains in-situ temperature and salinity profiles from different data types. The latest release CORA3 covers the period 1990 to 2010. Several tests have been developed to ensure a homogeneous quality control of the dataset and to meet the requirements of the physical ocean reanalysis activities (assimilation and validation). Improved tests include some simple tests based on comparison with climatology and a model background check based on a global ocean reanalysis. Visual quality control is performed on all suspicious temperature and salinity profiles identified by the tests, and quality...
Tipo: Text
Ano: 2013
URL: http://archimer.ifremer.fr/doc/00117/22799/20606.pdf

Utilisation des sondes NKE-STPS sur le voilier Fleur Australe (juin 2010-mars 2013)
Provedor de dados: 5
Autores: Desprez De Gesincourt, Floriane; Hamon, Michel; Branellec, Pierre; Gaillard, Fabienne.
Measurements of salinity by volontary observing ships are complementary of the measurements performed by the research vessels and represent a significant contribution to the global ocean observing networks. The Laboratoire de Physique des Océans (LPO) has tested four NKE-STPS sensors developped for the RECOPESCA project in collaboration with sailor Philippe Poupon. The sensors have been operating for 3 navigation seasons on board saling ship Fleur Australe. This reports synthesizes the informations related to the preparation, installation and checking of the sensors.
Tipo: Text
Ano: 2013
URL: http://archimer.ifremer.fr/doc/00156/26696/24764.pdf

Compte rendu de la campagne RREX 2015. N/O Thalassa 5 juin 2015 - 10 Juillet 2015
Provedor de dados: 5
Autores: Thierry, Virginie; Branellec, Pierre; Leizour, Stephane; Hamon, Michel.
Tipo: Text
Ano: 2015
URL: http://archimer.ifremer.fr/doc/00300/41154/40345.pdf

From Observation to Information and Users: The Copernicus Marine Service Perspective
Provedor de dados: 5
Autores: Le Traon, Pierre-yves; Reppucci, Antonio; Alvarez Fanjul, Enrique; Aouf, Lotfi; Behrens, Arno; Belmonte, Maria; Bentamy, Abderrahim; Bertino, Laurent; Brando, Vittorio Ernesto; Kreiner, Matilde Brandt; Benkiran, Mounir; Carval, Thierry; Ciliberti, Stefania A.; Claustre, Hervé; Clementi, Emanuela; Coppini, Giovanni; Cossarini, Gianpiero; De Alfonso Alonso-muñoyerro, Marta; Delamarche, Anne; Dibarboure, Gerald; Dinessen, Frode; Drevillon, Marie; Drillet, Yann; Faugere, Yannice; Fernández, Vicente; Fleming, Andrew; Garcia-hermosa, M. Isabel; Sotillo, Marcos García; Garric, Gilles; Gasparin, Florent; Giordan, Cedric; Gehlen, Marion; Gregoire, Marilaure L.; Guinehut, Stephanie; Hamon, Michel; Harris, Chris; Hernandez, Fabrice; Hinkler, Jørgen B.; Hoyer, Jacob; Karvonen, Juha; Kay, Susan; King, Robert; Lavergne, Thomas; Lemieux-dudon, Benedicte; Lima, Leonardo; Mao, Chongyuan; Martin, Matthew J; Masina, Simona; Melet, Angelique; Buongiorno Nardelli, Bruno; Nolan, Glenn; Pascual, Ananda; Pistoia, Jenny; Palazov, Atanas; Piolle, Jean-francois; Pujol, Marie Isabelle; Pequignet, Anne Christine; Peneva, Elisaveta; Pérez Gómez, Begoña; Petit De La Villeon, Loic; Pinardi, Nadia; Pisano, Andrea; Pouliquen, Sylvie; Reid, Rebecca; Remy, Elisabeth; Santoleri, Rosalia; Siddorn, John; She, Jun; Staneva, Joanna; Stoffelen, Ad; Tonani, Marina; Vandenbulcke, Luc; Von Schuckmann, Karina; Volpe, Gianluca; Wettre, Cecilie; Zacharioudaki, Anna.
The Copernicus Marine Environment Monitoring Service (CMEMS) provides regular and systematic reference information on the physical and biogeochemical ocean and sea-ice state for the global ocean and the European regional seas. CMEMS serves a wide range of users (more than 15,000 users are now registered to the service) and applications. Observations are a fundamental pillar of the CMEMS value-added chain that goes from observation to information and users. Observations are used by CMEMS Thematic Assembly Centres (TACs) to derive high-level data products and by CMEMS Monitoring and Forecasting Centres (MFCs) to validate and constrain their global and regional ocean analysis and forecasting systems. This paper presents an overview of CMEMS, its evolution,...
Tipo: Text
Palavras-chave: Ocean; Observing systems; Satellite; In situ; Data assimilation; Services.
Ano: 2019
URL: https://archimer.ifremer.fr/doc/00498/60983/64389.pdf

A surface kinematics buoy (SKIB) for wave–current interaction studies
Provedor de dados: 5
Autores: Veras Guimaraes, Pedro; Ardhuin, Fabrice; Sutherland, Peter; Accensi, Mickael; Hamon, Michel; Perignon, Yves; Thomson, Jim; Benetazzo, Alvise; Ferrant, Pierre.
Global navigation satellite systems (GNSSs) and modern motion-sensor packages allow the measurement of ocean surface waves with low-cost drifters. Drifting along or across current gradients provides unique measurements of wave–current interactions. In this study, we investigate the response of several combinations of GNSS receiver, motion-sensor package and hull design in order to define a prototype “surface kinematics buoy” (SKIB) that is particularly optimized for measuring wave–current interactions, including relatively short wave components that are important for air–sea interactions and remote-sensing applications. The comparison with existing Datawell Directional Waverider and Surface Wave Instrument Float with Tracking (SWIFT) buoys, as well as...
Tipo: Text
Ano: 2018
URL: https://archimer.ifremer.fr/doc/00470/58136/60605.pdf