Consulta: creatorFacets:"Malardé, Damien"
Registros recuperados: 2
Data/hora: 07/06/2024 03:35:06

Développement et essais d’un salinomètre optique pour l’océanographie
Provedor de dados: 5
Autores: Le Menn, Monique; Malardé, Damien; David, Arnaud; Brault, Patrice; Grosso, Philippe; De Bougrenet De La Tocnaye, Jean-louis; Le Reste, Serge; Podeur, Christian.
Salinity is the essential parameter for ocean dynamics studies. Its definition and using in the equations used to calculate the thermodynamic properties of seawater, were revised in 2010, opening the possibility of new sensors developments. In this context, NOSS (NKE Optical Salinity Sensor) has emerged as one of the first underwater instrument for in situ refractive index measurement in the past years open up the scope of possibilities to access to density parameter. This achievement is the fruit of the cooperation between several institutions and the fruit of several years of developments and trials. NOSS sensor is designed to be deployed in coastal environment and open-ocean waters up to 2000m, especially on profiling floats of the Argo network.
Tipo: Text
Palavras-chave: Salinity; Density; Ocean; Seawater; Refractive index; Sensor.
Ano: 2016
URL: https://archimer.ifremer.fr/doc/00664/77601/79616.pdf

Preparing the New Phase of Argo: Technological Developments on Profiling Floats in the NAOS Project
Provedor de dados: 5
Autores: André, Xavier; Le Traon, Pierre-yves; Le Reste, Serge; Dutreuil, Vincent; Leymarie, Edouard; Malardé, Damien; Marec, Claudie; Sagot, Jérôme; Amice, Martin; Babin, Marcel; Claustre, Hervé; David, Arnaud; D’ortenzio, Fabrizio; Kolodziejczyk, Nicolas; Lagunas, José Luis; Le Menn, Marc; Moreau, Bertrand; Nogré, David; Penkerc’h, Christophe; Poteau, Antoine; Renaut, Corentin; Schaeffer, Christophe; Taillandier, Vincent; Thierry, Virginie.
The international array of profiling floats known as Argo is a major component of the global ocean- and climate-observing system. In 2010, the NAOS (Novel Argo Observing System) project was selected as part of France’s Equipex “Investissement d’Avenir” program. The objectives of NAOS were to consolidate the French contribution to the Argo core mission (global temperature and salinity measurements down to 2,000 m) as well as to develop the future generation of French Argo profiling floats and prepare the next phase of the Argo program with an extension to the deep ocean (Deep-Argo), biogeochemistry (BGC-Argo) and polar seas. This paper summarizes the main technological advances and at-sea validations carried out as part of NAOS: development of a deep (4,000...
Tipo: Text
Palavras-chave: Ocean; Argo; Global observing system; Profiling float; Deep; Biogeochemistry; Under-ice; Float technology.
Ano: 2020
URL: https://archimer.ifremer.fr/doc/00658/77029/78314.pdf