Consulta: creatorFacets:"Milani,Adhemar P."
Registros recuperados: 4
Data/hora: 12/06/2024 04:45:26

Granjas leiteiras na região de Ribeirão Preto - SP
Provedor de dados: 70
Autores: Milani,Adhemar P.; Souza,Fernando A. De.
Nas atividades de exploração leiteira, as construções para os animais são fundamentais e de suma importância no processo de produção. Sendo assim, suas concepções devem basear-se em soluções técnicas e econômicas, que ofereçam condições eficientes e funcionais. O objetivo deste trabalho foi realizar um levantamento sobre as principais características de granjas leiteiras localizadas em municípios paulistas próximos a Ribeirão Preto e no sul de Minas Gerais e recomendar soluções, com base na literatura, para a execução de projeto para a região de Ribeirão Preto-SP. O trabalho foi desenvolvido com base em estudos teóricos e observações in loco, considerando as seguintes construções: galpão de estabulação livre; bezerreiro; sala de ordenha e seus anexos...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Construções rurais; Bovinocultura de leite; Granjas leiteiras.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000400018

Natural shading and productivity index of broiler chickens
Provedor de dados: 70
Autores: Souza,Fernando A.; Milani,Adhemar P.
The appropriate use of natural resources in the design of broiler houses provides a reduction in farming operating costs and optimization of production conditions. Therefore, the natural shading around the broiler house can be an alternative for improving internal conditions of comfort. This study verified the efficiency of natural shading in the broiler productivity index (PI) in East-West oriented commercial housings. The PI of 32 commercial broiler houses in five flocks divided throughout a year was compared. The sheds had the same management, density and the same structural features, except from tree shading: on the North face; on the South face; on both faces and without shading. It was observed that broiler house in East-West direction with shading...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Tree-shading; Ambience; Broiler houses; Broiler industry.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000300601

Evaluation of roof slope and exposure with different roofing materials in reduced models of animal production facilities in spring and summer
Provedor de dados: 70
Autores: Melo,Thiago V.; Furlan,Renato L.; Milani,Adhemar P.; Buzanskas,Marcos E.; Mota,Diego A.
The present study was conducted at the Department of Rural Engineering and the Department of Animal Morphology and Physiology of FCAV/Unesp, Jaboticabal, SP, Brazil. The objective was to verify the influence of roof slope, exposure and roofing material on the internal temperature of reduced models of animal production facilities. For the development of the research, 48 reduced and dissemble models with dimensions 1.00 × 1.00 × 0.50 m were used. The roof was shed-type, and the models faced to the North or South directions, with 24 models for each side of exposure. Ceramic, galvanized-steel and fibro tiles were used to build the roofs. Slopes varied between 20, 30, 40 and 50% for the ceramic tile and 10, 30, 40 and 50% for the other two. Inside the models,...
Tipo: Info:eu-repo/semantics/other
Palavras-chave: Ambience; Heat; Shed.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000600001

Estudo granulométrico de grãos de soja normal e transgênico
Provedor de dados: 70
Autores: Milani,Adhemar P.; Bidóia,Vitor S.; Perecin,Dilermando.
Este trabalho foi desenvolvido com o propósito de estudar o comportamento granulométrico de grãos de soja em função da variação do teor de água. A pesquisa foi realizada com seis variedades, sendo duas transgênicas e quatro comuns, com os teores de água de 10%, 12%, 15%, 20% b.s. A granulometria foi determinada utilizando-se de seis subamostras de 120 grãos para cada teor de água, e as suas dimensões (comprimento, largura e espessura) obtidas por meio de paquímetro digital. Os resultados indicaram que cada variedade de soja comportou-se de maneira diferenciada e que as comuns tiveram comportamento granulométrico diferenciado das transgênicas.
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Granulometria; Teor de água; Variedades de soja.
Ano: 2009
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162009000400015