Consulta: creatorFacets:"OBETTA, SAMUEL E."
Registros recuperados: 1
Data/hora: 11/06/2024 08:19:00

Effect of Expeller Press Parameters on Fish Oil Extraction
Provedor de dados: 111
Autores: BAKO, TANKO; UMOGBAI, VICTOR I.; OBETTA, SAMUEL E.
An investigation was carried out on the effect of expeller press parameters such as choke clearances (1, 2 and 3 mm), screw clearances (1, 2 and 3 mm) and screw (worm) shaft speeds (50, 60 and 70 rpm) on fish oil extraction. The oil extraction rate and extraction efficiency had a negative relationship with choke clearances and screw clearances but had a positive relationship with screw (worm) shaft speeds. The oil extraction rate and extraction efficiency were found to decrease with increase in choke clearances and also decreased with increase in screw clearances. Increase in screw (worm) shaft speeds from 50 to 70 rpm was observed to increase oil extraction rate and extraction efficiency. The extraction loss had a positive relationship with choke...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Fish oil; Extraction; Expeller; Parameters; Optimize.
Ano: 2018
URL: http://www.cigrjournal.org/index.php/Ejounral/article/view/4869