Consulta: creatorFacets:"Pereira,André B."
Registros recuperados: 3
Data/hora: 05/06/2024 14:12:22

Ajuste do método de Priestley-Taylor às condições climáticas locais
Provedor de dados: 70
Autores: Villa Nova,Nilson A.; Pereira,André B.
A sustentabilidade da agricultura irrigada depende primariamente do manejo eficiente da irrigação, de modo a aumentar a produtividade primária de uma cultura em determinada localidade. A eficiência no uso de água pode ser melhorada pelo próprio esquema de irrigação adotado, sendo essencialmente governado pelas condições climáticas. O planejamento da irrigação e a tomada de decisão são funções do conhecimento da demanda evaporativa da atmosfera, sendo expressa pela demanda potencial (ETo). Em geral, quase todos os métodos de estimativa de ETo reportados na literatura referem-se a valores diários, incluindo-se nessa situação as perdas noturnas de evaporação, as quais serão expressivas apenas em alguns dias após a chuva ou irrigação. Desenvolveu-se, no...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Balanço de energia; Modelagem; Demanda atmosférica.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000200007

Validation study of an overall radiation balance estimation method under Ponta Grossa (PR) Brazil weather conditions
Provedor de dados: 70
Autores: Beruski,Gustavo C.; Pereira,André B.
Radiation balance is the fraction of incident solar radiation upon earth surface which is available to be used in several natural processes, such as biological metabolism, water loss by vegetated surfaces, variation of temperature in farming systems and organic decomposition. The present study aimed to assess and validate the performance of two estimation models for Rn in Ponta Grossa city, Paraná State, Brazil. To this end, during the period of 04/01/2008 to 04/30/2011, from radiometric data collected by an automatic weather station set at the Experimental Station, of the State University of Ponta Grossa. We performed a linear regression study by confrontation between measurements made through radiometric balance and Rn estimates obtained from Brunt...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Overall radiation balance; Bowen ratio; Global solar radiation; Modeling; Solar radiometry.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000300010

Estimation of the potential evapotranspiration by a simplified penman method
Provedor de dados: 70
Autores: Villa Nova,Nilson A.; Miranda,Jarbas H. de; Pereira,André B.; Silva,Késia O. da.
The numerous methods for calculating the potential or reference evapotranspiration (ETo or ETP) almost always do for a 24-hour period, including values of climatic parameters throughout the nocturnal period (daily averages). These results have a nil effect on transpiration, constituting the main evaporative demand process in cases of localized irrigation. The aim of the current manuscript was to come up with a model rather simplified for the calculation of diurnal daily ETo. It deals with an alternative approach based on the theoretical background of the Penman method without having to consider values of aerodynamic conductance of latent and sensible heat fluxes, as well as data of wind speed and relative humidity of the air. The comparison between the...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Crop water use; Bowen ratio; Energy balance.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000300007