Consulta: creatorFacets:"Pereira Ribeiro, Danilo"
Registros recuperados: 1
Data/hora: 10/06/2024 17:45:04

ANALYSIS OF SPATIAL VARIABILITY OF CHEMICAL ATTRIBUTES OF SOIL IN NUTRIENT REMOVAL AND PRODUCTIVITY BRACHIARIA HUMIDICULA CULTIVATED IN SEWAGE TREATMENT RAMPS SANITARY OPERATING CONDITIONS IN REAL
Provedor de dados: 107
Autores: Nobre Santana, Rodrigo; Araújo Marques, Marcus Vinícius; Gomes Silva, Cláudio; Pereira Ribeiro, Danilo.
In Brazil, the sewage treatment system in runoff ramps was implemented by some sanitation companies for being low cost and provide similar treatment efficiency or greater than those obtained by conventional methods, provided that it is properly up kept. This work aimed to evaluate the spatial variability of soil chemical attributes, removing nutrients and the productivity of Brachiaria humidicula ramp runoff for sewage treatment. Ramps working in the municipality of Januária/MG, receive effluent from a primary treatment unit, an upflow anaerobic sludge blanket (UASB) which before passed through preliminary treatment (solid removal). 24 samples of soil and plant tissue were collected into a mesh mounted on the ramps. The pH, electric conductivity (EC), the...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Recursos Hídricos e Ambientais Água residuária; Características do solo; Remoção de nutrientes.
Ano: 2017
URL: http://www.seer.ufv.br/seer/index.php/reveng/article/view/735