Consulta: creatorFacets:"RODRIGUES,DIULIA C.Q."
Registros recuperados: 1
Data/hora: 02/06/2024 14:22:55

Dynamic Analysis of the Temperature and the Concentration Profiles of an Industrial Rotary Kiln Used in Clinker Production
Provedor de dados: 42
Autores: RODRIGUES,DIULIA C.Q.; SOARES JUNIOR,ATÍLIO P.; COSTA JUNIOR,ESLY F.; COSTA,ANDRÉA O.S.
ABSTRACT Cement is one of the most used building materials in the world. The process of cement production involves numerous and complex reactions that occur under different temperatures. Thus, there is great interest in the optimization of cement manufacturing. Clinker production is one of the main steps of cement production and it occurs inside the kiln. In this paper, the dry process of clinker production is analysed in a rotary kiln that operates in counter flow. The main phenomena involved in clinker production is as follows: free residual water evaporation of raw material, decomposition of magnesium carbonate, decarbonation, formation of C3A and C4AF, formation of dicalcium silicate, and formation of tricalcium silicate. The main objective of this...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Clinker; Dynamic analysis; Mathematical modelling; Rotary kiln.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0001-37652017000603123