Consulta: creatorFacets:"Steyer, Jean-philippe"
Registros recuperados: 2
Data/hora: 10/06/2024 07:44:13

Importance of ecological interactions during wastewater treatment using High Rate Algal Ponds under different temperate climates
Provedor de dados: 5
Autores: Galès, Amandine; Bonnafous, Anaïs; Carré, Claire; Jauzein, Vincent; Lanouguère, Elodie; Le Floc'H, Emilie; Pinoit, Joanna; Poullain, Clothilde; Roques, Cécile; Sialve, Bruno; Simier, Monique; Steyer, Jean-philippe; Fouilland, Eric.
Several studies focused on wastewater treatment in High Rate Algal Ponds (HRAP) suggest that highly variable climatic conditions cause large variations of microalgal biomass productivity. In the present study, we show that similar carbon, nitrogen and phosphorus removal efficiencies were reached in different HRAPs treating urban wastewaters located in two different temperate (Mediterranean and oceanic) climates. Furthermore, similar ecological successions were observed in these HRAPs. During the start-up phase, the consumption of organic matter by detritivores, already present in the wastewater, appears to be necessary for the microalgae to grow within two weeks in spring. The growth of the rapid-growing species, Chlorella sp., followed by the...
Tipo: Text
Palavras-chave: Microalgae; Predators; Bacteria; Urban effluents; Ammonia and phosphate removal.
Ano: 2019
URL: https://archimer.ifremer.fr/doc/00490/60210/63713.pdf

Carbon conversion efficiency and population dynamics of a marine algae–bacteria consortium growing on simplified synthetic digestate: First step in a bioprocess coupling algal production and anaerobic digestion
Provedor de dados: 5
Autores: Vasseur, Christophe; Bougaran, Gael; Garnier, Matthieu; Hamelin, Jérôme; Leboulanger, Christophe; Le Chevanton, Myriam; Mostajir, Behzad; Sialve, Bruno; Steyer, Jean-philippe; Fouilland, Eric.
Association of microalgae culture and anaerobic digestion seems a promising technology for sustainable algal biomass and biogas production. The use of digestates for sustaining the growth of microalgae reduces the costs and the environmental impacts associated with the substantial algal nutrient requirements. A natural marine algae–bacteria consortium was selected by growing on a medium containing macro nutrients (ammonia, phosphate and acetate) specific of a digestate, and was submitted to a factorial experimental design with different levels of temperature, light and pH. The microalgal consortium reached a maximum C conversion efficiency (i.e. ratio between carbon content produced and carbon supplied through light photosynthetic C conversion and acetate)...
Tipo: Text
Palavras-chave: Optimization; Nannochloris; Heterotrophic bacteria; Anaerobic digestion; Bioenergy.
Ano: 2012
URL: http://archimer.ifremer.fr/doc/00085/19642/17419.pdf