Consulta: subjectFacets:"2D/3D modeling"
Registros recuperados: 1
Data/hora: 05/06/2024 18:08:04

2D and 3D seismic simulation for fault modeling: exploratory revision from the Gullfaks field
Provedor de dados: 5
Autores: Siddiqui, Numair A.; Mathew, Manoj. J.; Menier, David; Hassaan, M.
2D and 3D seismic data have emerged as a key tool in the oil and gas industry to visualize and understand subsurface morphology and boundaries. In addition to providing excellent structural images, the dense sampling of 2D and 3D survey can sometimes make it possible to map reservoir quality and the distribution of hydrocarbon with well-marked limitations. Here we use 2D and 3D seismic data to map and interpret basic structures and fault lines to construct 2D and 3D base fault models of the Gullfaks field, while avoiding common pitfalls. This work also highlights important concepts and principles that allow selection, interpretation and simulation of particular areas containing hydrocarbon traps through the comparison of different maps such as time...
Tipo: Text
Palavras-chave: Seismic attributes; Fault interpretation; Horizon attributes maps; 2D/3D modeling; Gullfaks field.
Ano: 2017
URL: https://archimer.ifremer.fr/doc/00638/75035/75704.pdf