Consulta: subjectFacets:"Corn cobs"
Registros recuperados: 2
Data/hora: 12/06/2024 11:59:29

Armazenamento de espigas de milho em paiois.
Provedor de dados: 14
Autores: SAMPAIO, N. F.; OLIVEIRA, M. A. S.; VIANA, F. M. P.
Foi realizado um estudo preliminar de desempenho dos paióis como meios de armazenamento de espigas, foi feiot um teste comparativo entre um paiol de tela; outro de ripa e um terceiro de tábuas com paredes fechadas (não frestadas), sendo todos contruídos no campo experimental da UEPAE-Porto Velho, no início de 1982.
Tipo: Comunicado Técnico (INFOTECA-E)
Palavras-chave: Grain godowns; Rondônia; Amazônia Ocidental; Western Amazon.; Milho; Zea Mays; Espiga; Paiol.; Armazenamento; Storage.; Corn cobs.
Ano: 1983
URL: http://www.infoteca.cnptia.embrapa.br/infoteca/handle/doc/700196

Development of corn cob-based fuel briquettes
Provedor de dados: 111
Autores: tuates, andres MORALES.
The study aimed to determine the optimum proportion of corn cob biomass material and binder for fuel briquettes. Three (3) levels of percentage binding agent (10, 15, 20) and three (3) different particle size (&lt; 2.2mm, 2.2-3.2 and &gt;3.2mm) were used in the experiments. The physical and thermal properties of the fuel briquettes were characterized in terms of density, percent shatter resistance, breaking strength, thermal efficiency and burning time.Results showed that    twenty percent binding and a particle size of  &lt;2.2mm exhibited a high density of 0.30gm/ cc, the highest performance in the compression test with a value of 241.62 N  and good shatter resistance of 99.25 percent. Likewise, the thermal efficiency of the briquettes produced from the...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Corn cobs; Fuel briquettes; Physical and thermal properties; Burning time.
Ano: 2017
URL: http://www.cigrjournal.org/index.php/Ejounral/article/view/4089