Consulta: subjectFacets:"Harvest operations"
Registros recuperados: 1
Data/hora: 12/06/2024 06:46:24

Assessment of the soil compaction of two ultisols caused by logging operations
Provedor de dados: 90
Autores: Dias Junior,Moacir de Souza; Silva,Sérgio Ricardo; Santos,Nadívio Souza dos; Araujo-Junior,Cezar Francisco.
The impact of wood loads on bulk density and preconsolidation pressure and of harvester and forwarder traffic on rut depth, bulk density and preconsolidation pressure of two Ultisols were examined in this study. Our objective was to quantify the threshold beyond which significant soil compaction and rutting would occur. This study was carried out in the county of Eunápolis, state of Bahia, Brazil, (16 º 23 ' 17 '' S and 39 º 10 ' 06 '' W; altitude 80 m asl) in two Ultisols (PAd2 and PAd3) with different texture classes, in experimental areas with eucalypt plantation. The study involved measurements at the wood load site and machine driving at specific locations in the forest during logging operations. The treatments consisted of one harvester pass and, 8,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Rut depth; Soil compaction; Preconsolidation pressure; Harvest operations.
Ano: 2008
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-06832008000600004