Consulta: subjectFacets:"Irrigation moment"
Registros recuperados: 1
Data/hora: 01/06/2024 15:22:08

A rapid method for measuring soil water content in the field with a areometer
Provedor de dados: 63
Autores: Calbo,Adonai Gimenez.
The availability of a rapid method to evaluate the soil water content (U) can be an important tool to determine the moment to irrigate. The soil areometer consists of an elongated hydrostatic balance with a weighing pan, a graduated neck, a float and a pynometric flask. In this work an areometer was adapted to rapidly measure soil water content without the need of drying the soil. The expression U = (M A - M AD)/(M M -M A) was used to calculate the soil water content. In this equation M M is the mass to level the areometer with the pycnometric flask filled with water, M A the mass to level the areometer with a mass M M of soil in the pycnometer, the volume being completed with water, and similarly M AD the mass added to the pan to level the areometer with...
Tipo: Info:eu-repo/semantics/report
Palavras-chave: Hydrostatic balance; Irrigation moment; Pycnometer; Soil humidity.
Ano: 2002
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0103-90162002000400029