Consulta: subjectFacets:"Lead determination"
Registros recuperados: 1
Data/hora: 05/06/2024 15:22:25

3D-printed flow system for determination of lead in natural waters
Provedor de dados: 5
Autores: Mattio, Elodie; Robert-peillard, Fabien; Branger, Catherine; Puzio, Kinga; Margaillan, Andre; Brach-papa, Christophe; Knoery, Joel; Boudenne, Jean-luc; Coulomb, Bruno.
The development of 3D printing in recent years opens up a vast array of possibilities in the field of flow analysis. In the present study, a new 3D-printed flow system has been developed for the selective spectrophotometric determination of lead in natural waters. This system was composed of three 3D-printed units (sample treatment, mixing coil and detection) that might have been assembled without any tubing to form a complete flow system. Lead was determined in a two-step procedure. A preconcentration of lead was first carried out on TrisKem Pb Resin located in a 3D-printed column reservoir closed by a tapped screw. This resin showed a high extraction selectivity for lead over many tested potential interfering metals. In a second step, lead was eluted by...
Tipo: Text
Palavras-chave: Lead determination; 3D-printed MPFS system; Stereolithography; Natural waters.
Ano: 2017
URL: https://archimer.ifremer.fr/doc/00377/48770/49290.pdf