Consulta: subjectFacets:"Offshore"
Registros recuperados: 18
Data/hora: 07/06/2024 10:29:08

Activités parapétrolières et paragazières offshore. Sous-région marine Mers celtiques. Evaluation initiale DCSMM.
Provedor de dados: 5
Autores: Guingand, Aurélien.
Tipo: Text
Palavras-chave: Mers celtiques; Activités parapétrolières; Activités paragazières; Offshore; Réglementation; Interaction avec le milieu.
Ano: 2012
URL: https://archimer.ifremer.fr/doc/00329/43988/43560.pdf

Description and modeling of polyurethane hydrolysis used as thermal insulation in oil offshore conditions
Provedor de dados: 5
Autores: Le Gac, Pierre-yves; Choqueuse, Dominique; Melot, D.
Polymers are widely used for passive thermal insulation coatings on steel pipe in offshore oil and gas production. In this industry, structures used in deep sea have to be reliable, as they are in service for more than 20 years in a very severe environment: sea water, hydrostatic pressure and temperature gradient. One of the main questions is how to test and predict the lifetime of such structures in the laboratory? This study presents one approach that has been developed to characterize and predict the degradation of polymers used as thermal insulation materials.  This paper is dedicated to polyurethane (polyether based) degradation in sea water at high temperature. Ageing has been performed in natural sea water under hydrostatic pressure at temperatures...
Tipo: Text
Palavras-chave: Polyurethane; Hydrolysis; Accelerated ageing; Sea water; Coating; Offshore.
Ano: 2013
URL: http://archimer.ifremer.fr/doc/00160/27132/25330.pdf

Activités parapétrolières et paragazières offshore. Sous-région marine Golfe de Gascogne. Evaluation initiale DCSMM.
Provedor de dados: 5
Autores: Guingand, Aurélien.
Tipo: Text
Palavras-chave: Golfe de Gascogne; Activités parapétrolières; Activités paragazières; Offshore; Réglementation; Interaction avec le milieu.
Ano: 2012
URL: https://archimer.ifremer.fr/doc/00330/44080/43651.pdf

Analysis of slope failures in submarine canyon heads: An example from the Gulf of Lions
Provedor de dados: 5
Autores: Sultan, Nabil; Gaudin, Mathieu; Berne, Serge; Canals, Miquel; Urgeles, Roger; Lafuerza, Sara.
To improve understanding of evolution of submarine canyons, a three-dimensional slope-stability model is applied to Bourcart Canyon in the western Gulf of Lions in the Mediterranean Sea. The model builds on previous work by Chen and others, and it uses the upper bound theorem of plasticity to calculate the factor of safety of a kinematically admissible failing mass. Examples of three-dimensional failure surfaces documented in the literature were used to test the model formulation. Model application to Bourcart Canyon employed the results of a detailed stratigraphic analyses based on data acquired by swath bathymetry, sub-bottom profiling, high-resolution seismic reflection surveys, and piston coring. The sediment layers were also characterized using...
Tipo: Text
Palavras-chave: Cascadia accretionary complex; Upper bound theorem; Stability analysis; Continental slope; Limit equilibrium; Western gulf; Offshore; Margin; Initiation; Sediment.
Ano: 2007
URL: http://archimer.ifremer.fr/doc/2007/publication-2410.pdf

Durability of polydicyclopentadiene under high temperature, high pressure and seawater (offshore oil production conditions)
Provedor de dados: 5
Autores: Le Gac, Pierre-yves; Choqueuse, Dominique; Paris, Marc; Recher, G.; Zimmer, Celine; Melot, D.
In the offshore industry polymer coatings are widely used to ensure thermal insulation of steel pipes, and to avoid over-cooling of the hot oil inside. Because of very severe service conditions (i.e. high temperature, high pressure and presence of seawater) and an expected life time of 20 years, durability of these coatings is a major issue for this industry. Polypropylene and polyurethane are often used for this application, nevertheless these polymers have some limitations in terms of processing time for polypropylene and maximum service temperature for polyurethane. Polycyclopentadiene (pDCPD) shows good processing characteristics and low thermal conductivity, so this polymer could be a good alternative coating in the offshore industry, but the...
Tipo: Text
Palavras-chave: Polydicyclopentadiene; Seawater; Accelerated ageing; Oxidation; Offshore; Field joint.
Ano: 2013
URL: http://archimer.ifremer.fr/doc/00114/22534/20233.pdf

The experience of offshore marine fish farming in France
Provedor de dados: 5
Autores: De La Pomelie, C; Paquotte, Philippe.
A natural endowment of three coast lines with different structures, of numerous rivers coming from mountainous regions and of different climatic conditions has enabled France to develop one of the first European aquaculture sectors in terms of volume with almost 300 000 tonnes in 1996. This development has been based on a wide range of species and on a wide range of techniques. Intensive marine fish farming has been developing during the last decade only, after many years of stagnation due to the lack of reliable technology for species adapted to French climate. Techniques of production are very diverse. Although earth ponds and race-ways are used only by 25% of the marine fish farms, this technique accounts for 40% of the production. On the contrary, many...
Tipo: Text
Palavras-chave: Technology; Cages; Offshore; Mediterranean; Aquaculture; SEM; Technologie; Cages; Offshore; Méditerranée; Aquaculture.
Ano: 1998
URL: http://archimer.ifremer.fr/doc/1998/acte-4011.pdf

Gullfaks C offshore operation: Use of an hybrid team in subsea construction work: The Gullfaks "C" and oseberg north projects (use of the ROV).
Provedor de dados: 5
Autores: Rougier, R.
Installation and tie-in using tig automatic hyperbaric welding of 3 expansion loops to the Gullfaks "C" gravity base platform at 220 meters in the Norwegian sector of the North Sea. Operation performed from a dynamically positioned diving support vessel using divers and construction ROV during the summer 1989. Facing the technological challenge created by the deep diving aspects, the technical difficulties of doing welding operation at this depth, and the tight commercial constraints, a review of the tasks was conducted to optimize and reduce the offshore time, leading to innovations in the procedures selected to perform the work: Use of a working ROV, assisted by an observation vehicle, to carry out subsea tasks traditionally reserved for construction...
Tipo: Text
Palavras-chave: Diving; Offshore structures; Robots; Divers; Welding underwater; Offshore engineering; Unmanned vehicles; Marine technology; Offshore.
Ano: 1990
URL: http://archimer.ifremer.fr/doc/1990/acte-1162.pdf

Activités parapétrolières et paragazières offshore. Sous-région marine Manche - Mer du Nord. Evaluation initiale DCSMM.
Provedor de dados: 5
Autores: Guingand, Aurélien.
Tipo: Text
Palavras-chave: Manche; Mer du Nord; Activités parapétrolières; Activités paragazières; Offshore; Réglementation; Interaction avec le milieu.
Ano: 2012
URL: https://archimer.ifremer.fr/doc/00328/43894/43467.pdf

Use of ROV's in operation of EAN underwater installation in the North Sea.
Provedor de dados: 5
Autores: Ricci, F.
The purpose of the paper is to present the state of the Art in use of ROV for assistance in offshore operations. This is done through a review of operations and gained experience during East Frigg Field diverless installation in 1988 and 10 years or under water Inspection, Maintenance and Repair (IMR) on all Fields operated by Elf Aquitaine Norge A/S (EAN). Basic requirements to the types of ROVs are given and the cost-efficiency of the operations are discussed. The potential for further development of the ROVs to replace divers for a large part of annual IMR tasks below water is addressed.
Tipo: Text
Palavras-chave: Steel structures; Detection; Cracks; Surveillance and enforcement; Pipelines; Offshore structures; Underwater inspection; Offshore operations; Marine technology; Offshore; Unmanned vehicles.
Ano: 1990
URL: http://archimer.ifremer.fr/doc/1990/acte-1164.pdf

Offshore mollusc production in the Mediterranean basin
Provedor de dados: 5
Autores: Danioux, Christian; Bompais, Xavier; Paquotte, Philippe; Loste, Claudine.
In the Mediterranean basin, offshore mollusc production takes place mainly in France and Italy. Its recent development stems from the limited potential of lagoons and ponds, and centres mainly on mussel production. Suspension culture technologies are described and compared with those used in the Atlantic. Some information is given on the production systems and a short economic study demonstrates the profitability of these shellfish farming activities, in spite of the many risks involved and their relatively low profit margins.
Tipo: Text
Palavras-chave: Méditerranée; Mer ouverte; Mytiliculture; Filières; Technologie; Économie; Mediterranean; Offshore; Mussel farming; Long lines; Technology; Economy.
Ano: 2000
URL: https://archimer.ifremer.fr/doc/00469/58076/60485.pdf

Life time prediction of polymer used as thermal insulation in offshore oil production conditions: Ageing on real structure and reliability of prediction
Provedor de dados: 5
Autores: Le Gac, Pierre-yves; Choqueuse, Dominique; Melot, D.; Melve, B.; Meniconi, L.
Polymers are widely used for passive thermal insulation coatings on steel pipe in offshore oil and gas production. In this industry, structures used in deep sea have to be reliable as they are in service for more than 20 years in a very severe environment: sea water, hydrostatic pressure, temperature. One of the main questions is how to test and predict the lifetime of such structures in the laboratory. This study presents one approach that has been developed to characterize and predict the degradation of polyurethanes used as thermal insulation materials.  Based on results obtained during accelerated ageing of the PU in sea water, a prediction of degradation through the thickness has been set up taking into account the temperature profile in the coating,...
Tipo: Text
Palavras-chave: Polyurethane; Life time prediction; Hydrolysis; Offshore; Thermal insulation; Durability.
Ano: 2014
URL: http://archimer.ifremer.fr/doc/00174/28572/26957.pdf

Production de mollusques en mer ouverte dans le bassin méditerranéen
Provedor de dados: 5
Autores: Danioux, Christian; Bompais, Xavier; Loste, C; Paquotte, Philippe.
In the Mediterranean basin, the offshore mollusc production takes place mainly in France and Italy. Its recent development is the consequence of the small size of lagoons and ponds, and it is principally centred on the mussel. The farming technologies on long lines are described and compared with those used in the Atlantic. Some information is given on the production systems and a short economic study demonstrates the profitability of these shell farming activities, in spite of the many risks involved, but also their relatively low profit margins. [NOT CONTROLLED OCR]
Tipo: Text
Palavras-chave: Economy; Technology; Long lines; Mussel farming; Offshore; Mediterranean; SEM; Économie; Technologie; Filières; Mytiliculture; Mer ouverte; Méditerranée.
Ano: 1998
URL: http://archimer.ifremer.fr/doc/1998/acte-4012.pdf

Seasonal changes of chemical contamination in coastal waters during sediment resuspension
Provedor de dados: 5
Autores: Bancon-montigny, Chrystelle; Gonzalez, Catherine; Delpoux, Sophie; Avenzac, Muriel; Spinelli, Sylvie; Mhadhbi, Takoua; Mejri, Kaouther; Hlaili, Asma Sakka; Pringault, Olivier.
The potential of remobilization of pollutants is a major problem for anthropogenic ecosystems, because even when the anthropogenic source of pollution is identified and removed, pollutants stored in sediments can be released into the water column and impact pelagic communities during sediment resuspension provoked by dredging, storms or bottom trawling. The objectives of the present study were to assess the changes observed in the chemical composition of the water column following resuspension of a polluted marine sediment and the consequences for the chemical composition of adjacent marine waters according to season. For that purpose, an experimental sediment resuspension protocol was performed on four distinct occasions, spring, summer, fall and winter,...
Tipo: Text
Palavras-chave: Lagoon; Offshore; Trace metal elements; Pesticides; PAHs; Enrichment factor; Elutriate.
Ano: 2019
URL: https://archimer.ifremer.fr/doc/00505/61620/65644.pdf

Activités parapétrolières et paragazières offshore. Sous-région marine Méditerranée occidentale. Evaluation initiale DCSMM.
Provedor de dados: 5
Autores: Guingand, Aurélien.
Tipo: Text
Palavras-chave: Méditerranée; Activités parapétrolières; Activités paragazières; Offshore; Réglementation; Interaction avec le milieu.
Ano: 2012
URL: https://archimer.ifremer.fr/doc/00331/44262/43831.pdf

A review of potential economic mineral resources in offshore Nigeria
Provedor de dados: 20
Autores: Ibe, A.C.
Previously published data and preliminary indications from research now in progress suggest the possible occurrence in offshore Nigeria of economically viable deposits of placer minerals (including heavy minerals), sand and gravel, phosphorite, glauconite, polymetalic manganese nodules etc.  In addition, new stratigraphic evidence indicates the existence of potentially rich petroleum plays associated with a Tertiary canyon system in water depths beyond the limits of present exploitation.  Based on the comparative geology of similar occurrences in better explored continental margins and ocean basins elsewhere, the possible origin, abundance and distribution of these resources are adduced.  A brief assessment of the technology relevant to their discovery and...
Tipo: Report
Palavras-chave: Economic feasibility; Offshore; Mineral resources.
Ano: 1982
URL: http://hdl.handle.net/1834/1207

Suivi de l’activite de la pêche hauturiere dans le gouvernorat de Medenine (sud de la Tunisie)
Provedor de dados: 20
Autores: Chaalia, N.; ben abdallah-Ben hadj Hmida, O.; Ben hadj Hmida, N.; Jarboui, O.
Ce travail représente une contribution à l'étude de l'activité de pêche hauturière dans le gouvernorat de Médenine, particulièrement, au niveau du port de Zarzis ; durant la période (juin 2005-juin 2006). Il consiste à réaliser, grâce à des enquêtes menées au port, deux types d'analyses : une analyse quantitative afin de déterminer les débarquements saisonniers moyens des espèces les plus débarquées par la pêche hauturière et une analyse qualitative pour établir les structures démographiques des espèces les plus exploitées dans la région. Les résultats obtenus ont montré que, durant la période d'étude, les principales espèces débarquées par la pêche hauturière sont la sardinelle, le maquereau, le saurel, le rouget blanc, le pageot, la thonine, la seiche et...
Tipo: Proceedings Paper
Palavras-chave: Quality analysis; Offshore; Fisheries.
Ano: 2011
URL: http://hdl.handle.net/1834/5006

EC Project: System of Industry Metocean data for the Offshore and Research Communities (SIMORC).
Provedor de dados: 20
Autores: Vladymyrov, Vladimir.
Metocean in situ data are an important category of oceanographic and marine data, comprising observed parameters like sea level, waves, currents, sea temperature, conductivity, air temperature, air pressure, and wind. A very substantial volume of metocean in situ data is collected by or under contract to major oil &amp; gas companies. This is done all over the world and over many years a large volume of data sets has been acquired, often at substantial cost. These data are currently managed by the metocean departments of the oil &amp; gas companies and stored in various formats. They are exchanged on a limited scale between the oil &amp; gas companies. Despite various industry co-operative joint projects, there is not yet a common awareness of available...
Tipo: Conference Material
Palavras-chave: Offshore; Research; Oil and gas industry; Research; Http://aims.fao.org/aos/agrovoc/c_6513.
Ano: 2007
URL: http://hdl.handle.net/1834/2852

Results of the Environmental Impact Assessment for the Saltpond Offshore Programme  -Plankton Baseline Study
Provedor de dados: 20
Autores: Yaqub, B.H.
A report on plankton baseline studies conducted in the Saltpond Oil Field, Ghana.
Tipo: Report
Palavras-chave: Phytoplankton; Zooplankton; Plankton; Ichthyoplankton; Offshore; Salt water; EIA (environmental impact assessment); Salt water; Plankton.
Ano: 2013
URL: http://hdl.handle.net/1834/5326